* Copyright © 2000, 2001, 2002 Linear Technology Corporation.   All rights reserved.
*
.model 1N914 D(Is=2.52n Rs=0.568 N=1.752 Cjo=4p M=.4 tt=20n Iave=200m Vpk=75 mfg=Motorola type=silicon )
.model 1N4148 D(Is=2.52n Rs=0.568 N=1.752 Cjo=4p M=.4 tt=20n Iave=200m Vpk=75 mfg=Motorola type=silicon )
.model MMSD4148 D(Is=2.52n Rs=0.568 N=1.752 Cjo=.64p M=.4 tt=5n Iave=200m Vpk=100 mfg=Onsemi type=silicon )
.model 1N5817 D(Is=31.7u Rs=0.051 N=1.373 Cjo=190p M=.3 Eg=.69 Xti=2 Iave=1 Vpk=20 mfg=Motorola type=Schottky)
.model 1N5818 D(Is=31.7u Rs=0.051 N=1.373 Cjo=160p M=.38 Eg=.69 Xti=2 Iave=1 Vpk=30 mfg=Motorola type=Schottky)
.model 1N5819 D(Is=31.7u Rs=0.051 N=1.373 Cjo=110p M=.35 Eg=.69 Xti=2 Iave=1 Vpk=40 mfg=Motorola type=Schottky)
.model BAT54 D(Is=.1u Rs=2.2 N=1 Cjo=12p M=.3 Eg=.69 Xti=2 Iave=300m Vpk=30 mfg=Vishay type=Schottky)
.model MBR0520L D(Is=82.5n Rs=0.115 N=.7228 Cjo=180p M=.63 Eg=.69 Xti=2 Iave=.5 Vpk=20 mfg=Motorola type=Schottky)
.model MBR0530L D(Is=1.55u Rs=0.0858 N=1.079 Cjo=180p Eg=.69 Xti=2 Iave=.5 Vpk=30 mfg=Motorola type=Schottky)
.model MBRS1100 D(Is=20.6u Rs=0.0079 N=2.303 Cjo=270p M=.575 Eg=.69 Xti=2 Iave=1 Vpk=100 mfg=Motorola type=Schottky)
.model MBRS130L D(Is=772n Rs=0.0299 N=.8442 Cjo=290p M=.7 Eg=.69 Xti=2 Iave=1 Vpk=30 mfg=Motorola type=Schottky)
.model MBRS140 D(Is=235n Rs=0.109 N=.7760 Cjo=160p M=.6 Eg=.69 Xti=2 Iave=1 Vpk=40 mfg=Motorola type=Schottky)
.model MBRS340 D(Is=22.6u Rs=0.042 N=1.094 Cjo=480p M=.61 Eg=.69 Xti=2 Iave=3 Vpk=40 mfg=Motorola type=Schottky)
.model MBRS360 D(Is=22.6u Rs=0.042 N=1.094 Cjo=480p M=.61 Eg=.69 Xti=2 Iave=3 Vpk=60 mfg=Motorola type=Schottky)
.model CMDSH2-3 D(Is=210nA Rs=0.5 N=1.09 Cjo=50p M=.5 Eg=.69 Xti=2 Iave=200m Vpk=30 mfg=Central type=Schottky)
.model MURS120 D(Is=33.8n Rs=0.0236 N=1.718 Cjo=45p M=.6 tt=45n Iave=1 Vpk=200 mfg=Motorola type=silicon )
.model MURS320 D(Is=1.06n Rs=0.0111 N=1.367 Cjo=135p M=.45 tt=45n Iave=3 Vpk=200 mfg=Motorola type=silicon )
.model MBR735 D(Is=159u Rs=0.02 N=1.76 Cjo=740p M=.6 Eg=.69 Xti=2 Iave=7.5 Vpk=35 mfg=Motorola type=Schottky)
.model MBR745 D(Is=159u Rs=0.02 N=1.76 Cjo=740p M=.6 Eg=.69 Xti=2 Iave=7.5 Vpk=45 mfg=Motorola type=Schottky)
.model BZX84C6V2L D(Is=1.5n Rs=.5 Cjo=185p nbv=3 bv=6.2 Ibv=1m Vpk=6.2 mfg=Motorola type=zener )
.model BZX84C8V2L D(Is=0.8n Rs=.5 Cjo=135p nbv=3 bv=8.2 Ibv=1m Vpk=8.2 mfg=Motorola type=zener )
.model BZX84C10L D(Is=0.6u Rs=.5 Cjo=150p nbv=5 bv=10 Ibv=1m Vpk=10 mfg=Motorola type=zener )
.model BZX84C12L D(Is=0.6u Rs=.5 Cjo=150p nbv=5 bv=12 Ibv=1m Vpk=12 mfg=Motorola type=zener )
.model BZX84C15L D(Is=0.6u Rs=.5 Cjo=110p nbv=6 bv=15 Ibv=1m Vpk=15 mfg=Motorola type=zener )
.model RB10L-40 D(Is=2.6uA Rs=0.0674 N=1.163 Cjo=180p M=.6 Eg=.69 Xti=2 Iave=1 Vpk=40 mfg=Rohm type=Schottky)
.model 1N750 D(Is=.88f Rs=.25 Cjo=175p M=.55 nbv=1.7 bv=4.7 Vj=.75 Isr=1.86n Nr=2 Ibv=20.245m Ibvl=1.96m Nbvl=15 Tbv1=-21.3u Vpk=4.7 mfg=Motorola type=zener)
.model MV2201 D(Is=1.365p Rs=1 Cjo=14.93p M=.4261 Vj=.75 Isr=16.02p Nr=2 Bv=25 Ibv=10u Vpk=25 mfg=Motorola type=varactor)
.model MBR0540 D(Is=9.11u Rs=0.121 N=1.33753 Eg=0.69 Xti=2 Cjo=194p Vj=0.25 M=.4 Iave=.5 Vpk=40 mfg=GI type=Schottky)
.model MUR460 D(Is=149n Rs=0.0384 N=2 EG=1.285 XTI=0.5 BV=800 IBV=1e-05 Cjo=126.4p Vj=1.34 M=0.52 tt=44.4n Iave=4 Vpk=600 mfg=GI type=silicon)
.model MBRB2545CT D(Is=19.4n Rs=0.01 N=0.733 Eg=0.718 Xti=0.535 Cjo=2.05n Vj=0.4 M=0.41 Iave=25 Vpk=45 mfg=GI type=Schottky)
.model MBR20100CT D(Is=10u Rs=0.005 N=1.5 Ikf=.3 Isr=10u Nr=3 Cjo=1e-11 Vj=0.7 Iave=10 Vpk=100 mfg=Motorola type=Schottky)
.model 30BQ060 D(Is=10u Rs=0.04 N=1.4 Cjo=180p Eg=.69 Xti=2 Iave=3 Vpk=60 mfg=International_Rectifier type=Schottky)
.model UPSC600 D(Is=2p Rs=0.33 N=1.5 Cjo=50p M=.3 Iave=1 Vpk=600 mfg=Microsemi type=SiC_Schottky)
.model NSPW500BS D(Is=0.27n Rs=5.65 N=6.79 Cjo=42p Iave=30m Vpk=5 mfg=Nichia type=LED)
.model QTLP690C D(Is=1e-22 Rs=6 N=1.5 Cjo=50p Iave=160m Vpk=5 mfg=Fairchild type=LED)
.model PMEG2020AEA D(Is=5.409u Rs=0.05676 N=1.02 Cjo=0.1908n M=0.4863 Eg=0.69 Xti=2 BV=22 IBV=50u Vj=0.3408 FC=0.5 Iave=2 Vpk=20 mfg=Philips type=Schottky)
.model PMEG2010EA D(Is=1.686u Rs=0.1249 N=1.015 Cjo=90.86p M=0.4542 Eg=0.69 Xti=2 BV=21 IBV=1u Vj=0.1939 FC=1 Iave=1 Vpk=20 mfg=Philips type=Schottky)
.model PMEG2010BEA D(Is=3.334u Rs=0.08222 N=0.9791 Cjo=0.1266n M=0.5 Eg=0.69 Xti=2 BV=22 IBV=0.0001 Vj=0.3619 FC=0.5 Iave=1 Vpk=20 mfg=Philips type=Schottky)
.model PMEG3010BEA D(Is=2.936u Rs=0.1166 N=0.9839 Cjo=0.1068n M=0.4948 Eg=0.69 Xti=2 BV=33 IBV=75u Vj=0.3459 FC=0.5 Iave=1 Vpk=30 mfg=Philips type=Schottky)
.model PMEG4010BEA D(Is=2.831u Rs=0.1975 N=0.9816 Cjo=84.37p M=0.4789 Eg=0.69 Xti=2 BV=44 IBV=50u Vj=0.3116 FC=0.5 Iave=1 Vpk=40 mfg=Philips type=Schottky)
.model PMEG2005AEA D(Is=3.334u Rs=0.08222 N=0.9791 Cjo=0.1266n M=0.5 Eg=0.69 Xti=2 BV=22 IBV=0.0001 Vj=0.3619 FC=0.5 Iave=0.5 Vpk=20 mfg=Philips type=Schottky)
.model PMEG3005AEA D(Is=2.936u Rs=0.1166 N=0.9839 Cjo=0.1068n M=0.4948 Eg=0.69 Xti=2 BV=33 IBV=75u Vj=0.3459 FC=0.5 Iave=0.5 Vpk=30 mfg=Philips type=Schottky)
.model PMEG4005AEA D(Is=2.831u Rs=0.1975 N=0.9816 Cjo=84.37p M=0.4789 Eg=0.69 Xti=2 BV=44 IBV=50u Vj=0.3116 FC=0.5 Iave=0.5 Vpk=40 mfg=Philips type=Schottky)
.model PMEG2010AEB D(Is=87.24u Rs=0.2728 N=0.9699 Cjo=29.99p M=0.3755 Eg=0.69 Xti=2 BV=22 IBV=0.0004 Vj=0.2604 FC=0.5 Iave=1 Vpk=20 mfg=Philips type=Schottky)
.model PMEG2005EB D(Is=0.9985u Rs=0.2146 N=0.9283 Cjo=61.05p M=0.4159 Eg=0.69 Xti=2 BV=32 IBV=0.001 Vj=0.1 FC=0.5 Iave=0.5 Vpk=20 mfg=Philips type=Schottky)
.model PMEG6010AED D(Is=0.5u Rs=0.3422 N=0.9751 Cjo=0.175n M=0.4725 Eg=0.69 Xti=2 BV=66 IBV=0.0004 Vj=0.3761 FC=0.5 Iave=1 Vpk=60 mfg=Philips type=Schottky)
.model PRLL5817 D(Is=2.119u Rs=0.0419 N=1.02 Cjo=0.252n M=0.5104 Eg=0.69 Xti=2 BV=1000 IBV=0.001 Vj=0.4792 FC=0.5 Iave=1 Vpk=20 mfg=Philips type=Schottky)
.model GSD2004W-V D(Is=1e-14 Rs=1.6 N=1 Cjo=5p tt=50n Iave=225m Vpk=300 mfg=Vishay type=silicon)
.model LXHL-BW02 D(Is=4.5e-20 Rs=0.85 N=2.6 Cjo=1.18n Iave=400mA mfg=Lumileds type=LED)
.MODEL DI_2W005G D ( IS=28.4n RS=21.1m BV=50.0 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W01G D ( IS=28.4n RS=21.1m BV=100 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=100V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W02G D ( IS=28.4n RS=21.1m BV=200 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=200V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W04G D ( IS=28.4n RS=21.1m BV=400 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=400V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W06G D ( IS=28.4n RS=21.1m BV=600 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=600V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W08G D ( IS=28.4n RS=21.1m BV=800 IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=800V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_2W10G D ( IS=28.4n RS=21.1m BV=1.00k IBV=5.00u CJO=29.6p M=0.333 N=1.95 TT=4.32u Vpk=1.00kV Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF005M D ( IS=4.42n RS=42.0m BV=50.0 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF005S D ( IS=4.42n RS=42.0m BV=50.0 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF01M D ( IS=4.42n RS=42.0m BV=100 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF01S D ( IS=4.42n RS=42.0m BV=100 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF02M D ( IS=4.42n RS=42.0m BV=200 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF02S D ( IS=4.42n RS=42.0m BV=200 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF04M D ( IS=4.42n RS=42.0m BV=400 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF04S D ( IS=4.42n RS=42.0m BV=400 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF06M D ( IS=4.42n RS=42.0m BV=600 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF06S D ( IS=4.42n RS=42.0m BV=600 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF08M D ( IS=4.42n RS=42.0m BV=800 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF08S D ( IS=4.42n RS=42.0m BV=800 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF10M D ( IS=4.42n RS=42.0m BV=1.00k IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF10S D ( IS=4.42n RS=42.0m BV=1.00k IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DF15005M D ( IS=2.06n RS=28.1m BV=50.0 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF15005S D ( IS=2.06n RS=28.1m BV=50.0 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1501M D ( IS=2.06n RS=28.1m BV=100 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1501S D ( IS=2.06n RS=28.1m BV=100 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1502M D ( IS=2.06n RS=28.1m BV=200 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1502S D ( IS=2.06n RS=28.1m BV=200 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1504M D ( IS=2.06n RS=28.1m BV=400 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1504S D ( IS=2.06n RS=28.1m BV=400 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1506M D ( IS=2.06n RS=28.1m BV=600 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1506S D ( IS=2.06n RS=28.1m BV=600 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1508M D ( IS=2.06n RS=28.1m BV=800 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1508S D ( IS=2.06n RS=28.1m BV=800 IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1510M D ( IS=2.06n RS=28.1m BV=1.00k IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_DF1510S D ( IS=2.06n RS=28.1m BV=1.00k IBV=10.0u CJO=65.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ15005 D ( IS=5.11u RS=3.43m BV=50.0 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=50.0V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1501 D ( IS=5.11u RS=3.43m BV=100 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=100V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1502 D ( IS=5.11u RS=3.43m BV=200 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=200V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1504 D ( IS=5.11u RS=3.43m BV=400 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=400V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1506 D ( IS=5.11u RS=3.43m BV=600 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=600V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1508 D ( IS=5.11u RS=3.43m BV=800 IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=800V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ1510 D ( IS=5.11u RS=3.43m BV=1.00k IBV=10.0u CJO=106p M=0.333 N=2.44 TT=4.32u Vpk=1.00kV Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ20005 D ( IS=15.1u RS=2.96m BV=50.0 IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=50.0V Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2002 D ( IS=15.1u RS=2.96m BV=200 IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=200V Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2004 D ( IS=15.1u RS=2.96m BV=400 IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=400V Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2006 D ( IS=15.1u RS=2.96m BV=600 IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=600V Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2008 D ( IS=15.1u RS=2.96m BV=800 IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=800V Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2010 D ( IS=15.1u RS=2.96m BV=1.00k IBV=10.0u CJO=111p M=0.333 N=2.84 TT=4.32u Vpk=1.00kV Iave=20.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBJ2510 D ( IS=379n RS=2.84m BV=1.00k IBV=10.0u CJO=146p M=0.333 N=2.07 TT=4.32u Vpk=1.00kV Iave=25.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBPC3506 D ( IS=162u RS=3.32m BV=600 IBV=5.00u CJO=477p M=0.333 N=3.01 TT=4.32u Vpk=600V Iave=35.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBU1002 D ( IS=1.71f RS=7.00m BV=200 IBV=5.00u CJO=133p M=0.333 N=0.900 TT=4.32u Vpk=200V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_GBU4005 D ( IS=23.3n RS=7.20m BV=50.0 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=50.0V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU401 D ( IS=23.3n RS=7.20m BV=100 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=100V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU402 D ( IS=23.3n RS=7.20m BV=200 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=200V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU404 D ( IS=23.3n RS=7.20m BV=400 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=400V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU406 D ( IS=23.3n RS=7.20m BV=600 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=600V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU408 D ( IS=23.3n RS=7.20m BV=800 IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=800V Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU410 D ( IS=23.3n RS=7.20m BV=1.00k IBV=5.00u CJO=148p M=0.333 N=1.80 TT=4.32u Vpk=1.00kV Iave=4.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU8005 D ( IS=17.8p RS=7.59m BV=50.0 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=50.0V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU801 D ( IS=17.8p RS=7.59m BV=100 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=100V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU802 D ( IS=17.8p RS=7.59m BV=200 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=200V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU804 D ( IS=17.8p RS=7.59m BV=400 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=400V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU806 D ( IS=17.8p RS=7.59m BV=600 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=600V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU808 D ( IS=17.8p RS=7.59m BV=800 IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=800V Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_GBU810 D ( IS=17.8p RS=7.59m BV=1.00k IBV=5.00u CJO=240p M=0.333 N=1.25 TT=4.32u Vpk=1.00kV Iave=8.00A mfg=DiodesInc type=silicon )
.MODEL DI_HD01 D ( IS=3.47n RS=42.6m BV=100 IBV=5.00u CJO=25.2p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=0.800A mfg=DiodesInc type=silicon )
.MODEL DI_HD02 D ( IS=3.47n RS=42.6m BV=200 IBV=5.00u CJO=25.2p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=0.800A mfg=DiodesInc type=silicon )
.MODEL DI_HD04 D ( IS=3.47n RS=42.6m BV=400 IBV=5.00u CJO=25.2p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=0.800A mfg=DiodesInc type=silicon )
.MODEL DI_HD06 D ( IS=3.47n RS=42.6m BV=600 IBV=5.00u CJO=25.2p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=0.800A mfg=DiodesInc type=silicon )
.MODEL DI_KBP005G D ( IS=39.2u RS=28.1m BV=50.0 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP01G D ( IS=39.2u RS=28.1m BV=100 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP02G D ( IS=39.2u RS=28.1m BV=200 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP04G D ( IS=39.2u RS=28.1m BV=400 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP06G D ( IS=39.2u RS=28.1m BV=600 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP08G D ( IS=39.2u RS=28.1m BV=800 IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP10G D ( IS=39.2u RS=28.1m BV=1.00k IBV=5.00u CJO=26.5p M=0.333 N=4.38 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_KBP2005G D ( IS=143n RS=21.1m BV=50.0 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP201G D ( IS=143n RS=21.1m BV=100 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=100V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP202G D ( IS=143n RS=21.1m BV=200 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=200V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP204G D ( IS=143n RS=21.1m BV=400 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=400V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP206G D ( IS=143n RS=21.1m BV=600 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=600V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP208G D ( IS=143n RS=21.1m BV=800 IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=800V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_KBP210G D ( IS=143n RS=21.1m BV=1.00k IBV=5.00u CJO=46.2p M=0.333 N=2.12 TT=4.32u Vpk=1.00kV Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC301 D ( IS=492n RS=14.1m BV=50.0 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC302 D ( IS=492n RS=14.1m BV=100 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC303 D ( IS=492n RS=14.1m BV=200 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC304 D ( IS=492n RS=14.1m BV=400 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC305 D ( IS=492n RS=14.1m BV=600 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=600V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC306 D ( IS=492n RS=14.1m BV=800 IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC307 D ( IS=492n RS=14.1m BV=1.00k IBV=10.0u CJO=102p M=0.333 N=2.45 TT=4.32u ) Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC601 D ( IS=2.37n RS=5.14m BV=50.0 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=50.0V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC602 D ( IS=2.37n RS=5.14m BV=100 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=100V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC603 D ( IS=2.37n RS=5.14m BV=200 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=200V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC604 D ( IS=2.37n RS=5.14m BV=400 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=400V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC605 D ( IS=2.37n RS=5.14m BV=600 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=600V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC606 D ( IS=2.37n RS=5.14m BV=800 IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=800V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_PBPC607 D ( IS=2.37n RS=5.14m BV=1.00k IBV=10.0u CJO=102p M=0.333 N=1.63 TT=4.32u Vpk=1.00kV Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_RH02 D ( IS=2.25n RS=0.100 BV=200 IBV=5.00u CJO=24.0p M=0.333 N=1.70 TT=216n Vpk=200V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_RH04 D ( IS=2.25n RS=0.100 BV=400 IBV=5.00u CJO=24.0p M=0.333 N=1.70 TT=216n Vpk=400V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_RH06 D ( IS=2.25n RS=0.100 BV=600 IBV=5.00u CJO=24.0p M=0.333 N=1.70 TT=360n Vpk=600V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_W005G D ( IS=8.63u RS=28.0m BV=50.0 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W01G D ( IS=8.63u RS=28.0m BV=100 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W02G D ( IS=8.63u RS=28.0m BV=200 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W04G D ( IS=8.63u RS=28.0m BV=400 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W06G D ( IS=8.63u RS=28.0m BV=600 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W08G D ( IS=8.63u RS=28.0m BV=800 IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_W10G D ( IS=8.63u RS=28.0m BV=1.00k IBV=5.00u CJO=22.5p M=0.333 N=3.21 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_1N4933 D ( IS=830n RS=34.0m BV=50.0 IBV=5.00u CJO=26.5p M=0.333 N=2.46 TT=288n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4934 D ( IS=830n RS=34.0m BV=100 IBV=5.00u CJO=26.5p M=0.333 N=2.46 TT=288n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4935 D ( IS=830n RS=34.0m BV=200 IBV=5.00u CJO=26.5p M=0.333 N=2.46 TT=288n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4936 D ( IS=830n RS=34.0m BV=400 IBV=5.00u CJO=26.5p M=0.333 N=2.46 TT=288n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4937 D ( IS=830n RS=34.0m BV=600 IBV=5.00u CJO=26.5p M=0.333 N=2.46 TT=288n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES1A D ( IS=123n RS=42.0m BV=50.0 IBV=5.00u CJO=18.5p M=0.333 N=2.12 TT=28.8n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES1B D ( IS=123n RS=42.0m BV=100 IBV=5.00u CJO=18.5p M=0.333 N=2.12 TT=28.8n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES1C D ( IS=123n RS=42.0m BV=150 IBV=5.00u CJO=18.5p M=0.333 N=2.12 TT=28.8n Vpk=150V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES1D D ( IS=123n RS=42.0m BV=200 IBV=5.00u CJO=18.5p M=0.333 N=2.12 TT=28.8n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES1G D ( IS=373n RS=64.3m BV=400 IBV=5.00u CJO=18.5p M=0.333 N=2.84 TT=28.8n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2A D ( IS=267n RS=21.0m BV=50.0 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2AA D ( IS=267n RS=21.0m BV=50.0 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2B D ( IS=267n RS=21.0m BV=100 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=100V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2BA D ( IS=267n RS=21.0m BV=100 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=100V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2C D ( IS=267n RS=21.0m BV=150 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=150V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2CA D ( IS=267n RS=21.0m BV=150 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=150V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2D D ( IS=267n RS=21.0m BV=200 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=200V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2DA D ( IS=267n RS=21.0m BV=200 IBV=5.00u CJO=83.5p M=0.333 N=1.70 TT=36.0n Vpk=200V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES2G D ( IS=3.92n RS=21.0m BV=400 IBV=5.00u CJO=83.5p M=0.333 N=1.95 TT=36.0n Vpk=400V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3A D ( IS=7.27p RS=22.4m BV=50.0 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3AB D ( IS=7.27p RS=22.4m BV=50.0 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3B D ( IS=7.27p RS=22.4m BV=100 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3BB D ( IS=7.27p RS=22.4m BV=100 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3C D ( IS=7.27p RS=22.4m BV=150 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=150V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3CB D ( IS=7.27p RS=22.4m BV=150 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=150V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3D D ( IS=7.27p RS=22.4m BV=200 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_ES3DB D ( IS=7.27p RS=22.4m BV=200 IBV=10.0u CJO=83.2p M=0.333 N=0.700 TT=36.0n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_MURB1610CT D ( IS=3.19n RS=3.67m BV=100 IBV=5.00u CJO=225p M=0.333 N=1.59 TT=36.0n Vpk=100V Iave=16.0A mfg=DiodesInc type=silicon )
.MODEL DI_MURB1620CT D ( IS=3.19n RS=3.67m BV=200 IBV=5.00u CJO=225p M=0.333 N=1.59 TT=36.0n Vpk=200V Iave=16.0A mfg=DiodesInc type=silicon )
.MODEL DI_MURS120 D ( IS=17.1n RS=20.6m BV=200 IBV=2.00u CJO=60.0p M=0.333 N=1.73 TT=36.0n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_MURS140 D ( IS=17.1n RS=20.6m BV=400 IBV=2.00u CJO=45.0p M=0.333 N=1.73 TT=72.0n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_MURS160 D ( IS=17.1n RS=20.6m BV=600 IBV=2.00u CJO=45.0p M=0.333 N=1.73 TT=72.0n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_MURS320 D ( IS=11.8n RS=7.89m BV=200 IBV=5.00u CJO=45.0p M=0.333 N=1.56 TT=36.0n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1001G D ( IS=5.00n RS=29.8m BV=50.0 IBV=5.00u CJO=27.8p M=0.333 N=1.72 TT=216n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1002G D ( IS=5.00n RS=29.8m BV=100 IBV=5.00u CJO=27.8p M=0.333 N=1.72 TT=216n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1003G D ( IS=5.00n RS=29.8m BV=200 IBV=5.00u CJO=27.8p M=0.333 N=1.72 TT=216n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1004G D ( IS=5.00n RS=29.8m BV=400 IBV=5.00u CJO=27.8p M=0.333 N=1.72 TT=216n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1005G D ( IS=5.00n RS=29.8m BV=600 IBV=5.00u CJO=19.9p M=0.333 N=1.72 TT=360n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1006G D ( IS=5.00n RS=29.8m BV=800 IBV=5.00u CJO=19.9p M=0.333 N=1.72 TT=720n Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR1007G D ( IS=5.00n RS=29.8m BV=1.00k IBV=5.00u CJO=19.9p M=0.333 N=1.72 TT=720n Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_PR6001 D ( IS=863n RS=12.6m BV=50.0 IBV=10.0u CJO=663p M=0.333 N=1.70 TT=216n Vpk=50.0V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1A D ( IS=948n RS=81.3m BV=50.0 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1AB D ( IS=948n RS=81.3m BV=50.0 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1B D ( IS=948n RS=81.3m BV=100 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1BB D ( IS=948n RS=81.3m BV=100 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1D D ( IS=948n RS=81.3m BV=200 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1DB D ( IS=948n RS=81.3m BV=200 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1G D ( IS=948n RS=81.3m BV=400 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1GB D ( IS=948n RS=81.3m BV=400 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=216n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1J D ( IS=948n RS=81.3m BV=600 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=360n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1JB D ( IS=948n RS=81.3m BV=600 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=360n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1K D ( IS=948n RS=81.3m BV=800 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=720n Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1KB D ( IS=948n RS=81.3m BV=800 IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=720n Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1M D ( IS=948n RS=81.3m BV=1.00k IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=720n Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS1MB D ( IS=948n RS=81.3m BV=1.00k IBV=5.00u CJO=27.7p M=0.333 N=2.48 TT=720n Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS2A D ( IS=169u RS=4.81m BV=50.0 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2AA D ( IS=169u RS=4.81m BV=50.0 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2B D ( IS=169u RS=4.81m BV=100 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2BA D ( IS=169u RS=4.81m BV=100 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2D D ( IS=169u RS=4.81m BV=200 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2DA D ( IS=169u RS=4.81m BV=200 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2G D ( IS=169u RS=4.81m BV=400 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2GA D ( IS=169u RS=4.81m BV=400 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=216n Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2J D ( IS=169u RS=4.81m BV=600 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=360n Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2JA D ( IS=169u RS=4.81m BV=600 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=360n Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2K D ( IS=169u RS=4.81m BV=800 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=720n Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2KA D ( IS=169u RS=4.81m BV=800 IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=720n Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2M D ( IS=169u RS=4.81m BV=1.00k IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=720n Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS2MA D ( IS=169u RS=4.81m BV=1.00k IBV=5.00u CJO=55.5p M=0.333 N=6.02 TT=720n Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_RS3A D ( IS=200n RS=25.4m BV=50.0 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3AB D ( IS=200n RS=25.4m BV=50.0 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3B D ( IS=200n RS=25.4m BV=100 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3BB D ( IS=200n RS=25.4m BV=100 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3D D ( IS=200n RS=25.4m BV=200 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3DB D ( IS=200n RS=25.4m BV=200 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3G D ( IS=200n RS=25.4m BV=400 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3GB D ( IS=200n RS=25.4m BV=400 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=216n Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3J D ( IS=200n RS=25.4m BV=600 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=360n Vpk=600V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3JB D ( IS=200n RS=25.4m BV=600 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=360n Vpk=600V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3K D ( IS=200n RS=25.4m BV=800 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=720n Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3KB D ( IS=200n RS=25.4m BV=800 IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=720n Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3M D ( IS=200n RS=25.4m BV=1.00k IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=720n Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_RS3MB D ( IS=200n RS=25.4m BV=1.00k IBV=5.00u CJO=92.5p M=0.333 N=2.23 TT=720n Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10AG D ( IS=1.42n RS=42.0m BV=50.0 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=50.4n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10BG D ( IS=1.42n RS=42.0m BV=100 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=50.4n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10CG D ( IS=1.42n RS=42.0m BV=150 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=50.4n Vpk=150V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10DG D ( IS=1.42n RS=42.0m BV=200 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=50.4n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10FG D ( IS=50.9p RS=75.5m BV=300 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=57.6n Vpk=300V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10GG D ( IS=50.9p RS=75.5m BV=400 IBV=10.0u CJO=139p M=0.333 N=1.70 TT=57.6n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10HG D ( IS=13.5u RS=30.9m BV=500 IBV=10.0u CJO=92.5p M=0.333 N=5.40 TT=72.0n Vpk=500V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_SF10JG D ( IS=13.5u RS=30.9m BV=600 IBV=10.0u CJO=92.5p M=0.333 N=5.40 TT=72.0n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_UF3001 D ( IS=70.7u RS=43.0u BV=50.0 IBV=10.0u CJO=139p M=0.333 N=4.27 TT=72.0n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_UF3002 D ( IS=70.7u RS=43.0u BV=100 IBV=5.00u CJO=139p M=0.333 N=4.27 TT=72.0n Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_UF3003 D ( IS=70.7u RS=43.0u BV=200 IBV=5.00u CJO=139p M=0.333 N=4.27 TT=72.0n Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_UF3004 D ( IS=9.58u RS=15.4m BV=400 IBV=5.00u CJO=139p M=0.333 N=3.45 TT=72.0n Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL Di_UF3005 D ( IS=4.50u RS=14.1m BV=600 IBV=10.0u CJO=92.5p M=0.333 N=4.29 TT=108n Vpk=600V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL Di_UF3006 D ( IS=4.50u RS=14.1m BV=800 IBV=10.0u CJO=92.5p M=0.333 N=4.29 TT=108n Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL Di_UF3007 D ( IS=4.50u RS=14.1m BV=1.00k IBV=10.0u CJO=92.5p M=0.333 N=4.29 TT=108n Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1A D ( IS=667n RS=72.0m BV=50.0 IBV=5.00u CJO=37.0p M=0.333 N=2.41 TT=72.0n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1B D ( IS=667n RS=72.0m BV=100 IBV=5.00u CJO=37.0p M=0.333 N=2.41 TT=72.0n Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1D D ( IS=667n RS=72.0m BV=200 IBV=5.00u CJO=37.0p M=0.333 N=2.41 TT=72.0n Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1G D ( IS=540p RS=0.116 BV=400 IBV=5.00u CJO=37.0p M=0.333 N=1.70 TT=72.0n Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1J D ( IS=709n RS=82.3m BV=600 IBV=5.00u CJO=18.5p M=0.333 N=3.23 TT=108n Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1K D ( IS=709n RS=82.3m BV=800 IBV=5.00u CJO=18.5p M=0.333 N=3.23 TT=108n Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_US1M D ( IS=709n RS=82.3m BV=1.00k IBV=5.00u CJO=18.5p M=0.333 N=3.23 TT=108n Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5711W D ( IS=315n RS=2.80 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=2.03 TT=1.44n Vpk=70.0V Iave=15.0mA mfg=DiodesInc type=silicon )
.MODEL DI_1N5711WS D ( IS=315n RS=2.80 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=2.03 TT=1.44n Vpk=70.0V Iave=15.0mA mfg=DiodesInc type=silicon )
.MODEL DI_1N6263W D ( IS=1.82u RS=2.80 BV=60.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=60.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-04 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-04T D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-05 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-05T D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-06 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40-06T D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40BRW D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40DW-04 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40DW-05 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40DW-06 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40T D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40TW D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40W D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40W-04 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40W-05 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS40W-06 D ( IS=6.12u RS=0.120 BV=40.0 IBV=200n CJO=5.00p M=0.333 N=2.61 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=silicon )
.MODEL DI_BAS70-04 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70-04T D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70-05 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70-05T D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70-06 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70-06T D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70BRW D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70DW-04 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70DW-05 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70DW-06 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70JW D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70T D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70TW D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70W D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70W-04 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70W-05 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAS70W-06 D ( IS=99.5p RS=0.600 BV=70.0 IBV=10.0u CJO=2.00p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=70.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_BAT42 D ( IS=2.46u RS=0.210 BV=30.0 IBV=500n CJO=13.3p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT42W D ( IS=87.5u RS=18.1m BV=30.0 IBV=500n CJO=8.88p M=0.333 N=3.51 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT42WS D ( IS=87.5u RS=18.1m BV=30.0 IBV=500n CJO=8.88p M=0.333 N=3.51 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT43W D ( IS=87.5u RS=18.1m BV=30.0 IBV=500n CJO=8.88p M=0.333 N=3.51 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT43WS D ( IS=87.5u RS=18.1m BV=30.0 IBV=500n CJO=8.88p M=0.333 N=3.51 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT46 D ( IS=603n RS=0.280 BV=100 IBV=5.00u CJO=7.96p M=0.333 N=1.70 TT=7.20n Vpk=100V Iave=0.150A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT46W D ( IS=603n RS=0.280 BV=100 IBV=5.00u CJO=7.96p M=0.333 N=1.70 TT=7.20n Vpk=100V Iave=0.150A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54 D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54A D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54ADW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54AT D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54AW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54BRW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54C D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54CDW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54CT D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54CW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54DW D ( IS=235n RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=1.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54JW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54S D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54SDW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54ST D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54SW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54T D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54TW D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54W D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT54WS D ( IS=34.9u RS=0.210 BV=30.0 IBV=2.00u CJO=13.3p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_QSBT40 D ( IS=500n RS=0.211 BV=30.0 IBV=2.00u CJO=10.0p M=0.333 N=1.70 TT=72.0n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_SD101A D ( IS=1.82u RS=2.80 BV=60.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=60.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101AW D ( IS=1.82u RS=2.80 BV=60.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=60.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101AWS D ( IS=230n RS=2.13 BV=60.0 IBV=200n CJO=2.00p M=0.333 N=1.96 TT=1.44n Vpk=60.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101B D ( IS=1.82u RS=2.80 BV=50.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=50.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101BW D ( IS=1.82u RS=2.80 BV=50.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=50.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101BWS D ( IS=1.82u RS=2.80 BV=50.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=50.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101C D ( IS=1.82u RS=2.80 BV=40.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=40.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101CW D ( IS=1.82u RS=2.80 BV=40.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=40.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD101CWS D ( IS=1.82u RS=2.80 BV=40.0 IBV=200n CJO=2.65p M=0.333 N=1.70 TT=1.44n Vpk=40.0V Iave=15.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SD103ASDM D ( IS=646n RS=0.120 BV=40.0 IBV=5.00u CJO=29.2 M=0.333 N=1.28 TT=14.4n Vpk=40.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103ATW D ( IS=646n RS=0.120 BV=40.0 IBV=5.00u CJO=29.2 M=0.333 N=1.28 TT=14.4n Vpk=40.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103AW D ( IS=8.65u RS=0.120 BV=40.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103AWS D ( IS=8.65u RS=0.120 BV=40.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=0.350A mfg=DiodesInc type=silicon )
.MODEL DI_SD103BW D ( IS=8.65u RS=0.120 BV=30.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=30.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103BWS D ( IS=8.65u RS=0.120 BV=30.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=30.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103CW D ( IS=8.65u RS=0.120 BV=20.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=20.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SD103CWS D ( IS=8.65u RS=0.120 BV=20.0 IBV=5.00u CJO=53.0p M=0.333 N=1.70 TT=14.4n Vpk=20.0V Iave=0.350A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM03MT40 D ( IS=309u RS=0.210 BV=40.0 IBV=1.00u CJO=2.65p M=0.333 N=6.81 TT=7.20n Vpk=40.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM03U40 D ( IS=16.5u RS=2.20 BV=30.0 IBV=500n CJO=2.59p M=0.333 N=2.92 TT=1.44n Vpk=30.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDM10M45SD D ( IS=290n RS=0.420 BV=45.0 IBV=1.00u CJO=10.6p M=0.333 N=1.28 TT=7.20n Vpk=45.0V Iave=0.100A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM10P45 D ( IS=745n RS=0.792 BV=45.0 IBV=1.00u CJO=11.2p M=0.333 N=1.39 TT=7.20n Vpk=45.0V Iave=0.100A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM10U45 D ( IS=26.8u RS=0.140 BV=40.0 IBV=1.00u CJO=10.6p M=0.333 N=2.45 TT=7.20n Vpk=40.0V Iave=0.300A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM20E40C D ( IS=3.15u RS=0.165 BV=40.0 IBV=70.0u CJO=39.8p M=0.333 N=1.16 TT=7.20n Vpk=40.0V Iave=0.400A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM20U30 D ( IS=59.4n RS=0.210 BV=30.0 IBV=150u CJO=19.9p M=0.333 N=0.700 TT=7.20n Vpk=30.0V Iave=0.200A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM20U40 D ( IS=4.32u RS=0.168 BV=40.0 IBV=5.00u CJO=39.8p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=0.250A mfg=DiodesInc type=Schottky )
.MODEL DI_SDM40E20LS D ( IS=54.8u RS=0.132 BV=20.0 IBV=250u CJO=199p M=0.333 N=1.34 TT=7.20n Vpk=20.0V Iave=0.400A mfg=DiodesInc type=Schottky )
.MODEL DI_SBMG0340L D ( IS=13.9u RS=2.57 BV=40.0 IBV=10.0u CJO=2.65p M=0.333 N=2.82 TT=1.44n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=silicon )
.MODEL DI_SBMG0340LA D ( IS=13.9u RS=2.57 BV=40.0 IBV=10.0u CJO=2.65p M=0.333 N=2.82 TT=1.44n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SBMG0340LC D ( IS=13.9u RS=2.57 BV=40.0 IBV=10.0u CJO=2.65p M=0.333 N=2.82 TT=1.44n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SBMG0340LS D ( IS=13.9u RS=2.57 BV=40.0 IBV=10.0u CJO=2.65p M=0.333 N=2.82 TT=1.44n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDMK0340L D ( IS=11.2u RS=3.64 BV=40.0 IBV=500n CJO=2.65p M=0.333 N=2.69 TT=4.32u Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDMP0340LAT D ( IS=16.5u RS=2.20 BV=40.0 IBV=1.00u CJO=2.65p M=0.333 N=2.92 TT=7.20n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDMP0340LCT D ( IS=16.5u RS=2.20 BV=40.0 IBV=1.00u CJO=2.65p M=0.333 N=2.92 TT=7.20n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDMP0340LST D ( IS=16.5u RS=2.20 BV=40.0 IBV=1.00u CJO=2.65p M=0.333 N=2.92 TT=7.20n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_SDMP0340LT D ( IS=16.5u RS=2.20 BV=40.0 IBV=1.00u CJO=2.65p M=0.333 N=2.92 TT=7.20n Vpk=40.0V Iave=30.0mA mfg=DiodesInc type=Schottky )
.MODEL DI_1N5819HW D ( IS=191u RS=42.0m BV=40.0 IBV=1.00m CJO=239p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B0520LW D ( IS=195u RS=49.4m BV=20.0 IBV=250u CJO=199p M=0.333 N=1.72 TT=7.20n Vpk=20.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_B0520WS D ( IS=1.96u RS=0.131 BV=20.0 IBV=250u CJO=170p M=0.333 N=0.907 TT=7.20u Vpk=20.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_B0530W D ( IS=47.4u RS=26.8m BV=30.0 IBV=130u CJO=225p M=0.333 N=1.66 TT=7.20n Vpk=30.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_B0530WS D ( IS=897u RS=72.9m BV=30.0 IBV=500u CJO=79.6p M=0.333 N=2.85 TT=14.4n Vpk=30.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_B0540W D ( IS=55.9p RS=0.125 BV=40.0 IBV=20.0u CJO=225p M=0.333 N=0.700 TT=14.4n Vpk=40.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_B1100 D ( IS=89.3u RS=42.2m BV=100 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=100V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B1100B D ( IS=89.3u RS=42.2m BV=100 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=100V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B1100LB D ( IS=20.0n RS=24.7m BV=100 IBV=500n CJO=225p M=0.333 N=1.22 TT=14.4n Vpk=100V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B120 D ( IS=39.6u RS=50.2m BV=20.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=20.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B120B D ( IS=39.6u RS=50.2m BV=20.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=20.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B130 D ( IS=39.6u RS=50.2m BV=30.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B130B D ( IS=39.6u RS=50.2m BV=30.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B130L D ( IS=188u RS=18.5m BV=30.0 IBV=1.00m CJO=331p M=0.333 N=1.65 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B130LAW D ( IS=407u RS=75.5m BV=30.0 IBV=1.00m CJO=119p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B130LB D ( IS=458u RS=28.0m BV=30.0 IBV=1.00m CJO=159p M=0.333 N=1.70 TT=14.4n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B140 D ( IS=39.6u RS=50.2m BV=40.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B140B D ( IS=39.6u RS=50.2m BV=40.0 IBV=500u CJO=265p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B140HB D ( IS=31.0u RS=42.1m BV=40.0 IBV=1.00m CJO=159p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B150 D ( IS=15.7u RS=42.0m BV=50.0 IBV=500u CJO=133p M=0.333 N=1.70 TT=7.20n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B150B D ( IS=15.7u RS=42.0m BV=50.0 IBV=500u CJO=133p M=0.333 N=1.70 TT=7.20n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B160 D ( IS=15.7u RS=42.0m BV=60.0 IBV=500u CJO=133p M=0.333 N=1.70 TT=7.20n Vpk=60.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B160B D ( IS=15.7u RS=42.0m BV=60.0 IBV=500u CJO=133p M=0.333 N=1.70 TT=7.20n Vpk=60.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B170 D ( IS=89.3u RS=42.2m BV=70.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=70.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B170B D ( IS=89.3u RS=42.2m BV=70.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=70.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B180 D ( IS=89.3u RS=42.2m BV=80.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=80.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B180B D ( IS=89.3u RS=42.2m BV=80.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=80.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B190 D ( IS=89.3u RS=42.2m BV=90.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=90.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B190B D ( IS=89.3u RS=42.2m BV=90.0 IBV=500n CJO=66.3p M=0.333 N=2.45 TT=7.20n Vpk=90.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B2100 D ( IS=746u RS=21.0m BV=100.0 IBV=500u CJO=179p M=0.333 N=2.87 TT=14.4n Vpk=100.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B220 D ( IS=7.98u RS=13.4m BV=20.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=20.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B220A D ( IS=7.98u RS=13.4m BV=20.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=20.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B230 D ( IS=7.98u RS=13.4m BV=30.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=30.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B230A D ( IS=7.98u RS=13.4m BV=30.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=30.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B240 D ( IS=7.98u RS=13.4m BV=40.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=40.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B240A D ( IS=7.98u RS=13.4m BV=40.0 IBV=500u CJO=370p M=0.333 N=1.13 TT=1.44n Vpk=40.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B250 D ( IS=6.08u RS=14.9m BV=50.0 IBV=500u CJO=370p M=0.333 N=1.55 TT=1.44n Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B250A D ( IS=6.08u RS=14.9m BV=50.0 IBV=500u CJO=370p M=0.333 N=1.55 TT=1.44n Vpk=50.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B260 D ( IS=6.08u RS=14.9m BV=60.0 IBV=500u CJO=370p M=0.333 N=1.55 TT=1.44n Vpk=60.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B260A D ( IS=6.08u RS=14.9m BV=60.0 IBV=500u CJO=370p M=0.333 N=1.55 TT=1.44n Vpk=60.0V Iave=2.00A mfg=DiodesInc type=silicon )
.MODEL DI_B270 D ( IS=746u RS=21.0m BV=70.0 IBV=500u CJO=179p M=0.333 N=2.87 TT=14.4n Vpk=70.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B280 D ( IS=746u RS=21.0m BV=80.0 IBV=500u CJO=179p M=0.333 N=2.87 TT=14.4n Vpk=80.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B290 D ( IS=746u RS=21.0m BV=90.0 IBV=500u CJO=179p M=0.333 N=2.87 TT=14.4n Vpk=90.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B3100 D ( IS=916u RS=14.1m BV=100 IBV=500u CJO=159p M=0.333 N=3.04 TT=14.4n Vpk=100V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B320 D ( IS=9.90n RS=14.0m BV=20.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=20.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B320A D ( IS=9.90n RS=14.0m BV=20.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=20.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B320B D ( IS=9.90n RS=14.0m BV=20.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=20.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B330 D ( IS=9.90n RS=14.0m BV=30.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=30.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B330A D ( IS=9.90n RS=14.0m BV=30.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=30.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B330B D ( IS=9.90n RS=14.0m BV=30.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=30.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B340 D ( IS=9.90n RS=14.0m BV=40.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B340A D ( IS=9.90n RS=14.0m BV=40.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B340B D ( IS=9.90n RS=14.0m BV=40.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B340LA D ( IS=1.15m RS=17.8m BV=40.0 IBV=2.00m CJO=411p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B340LB D ( IS=1.15m RS=17.8m BV=40.0 IBV=2.00m CJO=411p M=0.333 N=1.70 TT=14.4n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B350 D ( IS=9.90n RS=14.0m BV=50.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B350A D ( IS=9.90n RS=14.0m BV=50.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B350B D ( IS=9.90n RS=14.0m BV=50.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=50.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B360 D ( IS=9.90n RS=14.0m BV=60.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=60.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B360A D ( IS=9.90n RS=14.0m BV=60.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=60.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B360B D ( IS=9.90n RS=14.0m BV=60.0 IBV=500u CJO=464p M=0.333 N=0.775 TT=7.20n Vpk=60.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B370 D ( IS=916u RS=14.1m BV=70.0 IBV=500u CJO=159p M=0.333 N=3.04 TT=14.4n Vpk=70.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B380 D ( IS=916u RS=14.1m BV=80.0 IBV=500u CJO=159p M=0.333 N=3.04 TT=14.4n Vpk=80.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B390 D ( IS=916u RS=14.1m BV=90.0 IBV=500u CJO=159p M=0.333 N=3.04 TT=14.4n Vpk=90.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B520C D ( IS=617u RS=10.0m BV=20.0 IBV=500u CJO=497p M=0.333 N=1.70 TT=7.20n Vpk=20.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B530C D ( IS=617u RS=10.0m BV=30.0 IBV=500u CJO=497p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B540C D ( IS=617u RS=10.0m BV=40.0 IBV=500u CJO=497p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B550C D ( IS=66.7u RS=14.1m BV=50.0 IBV=500u CJO=497p M=0.333 N=1.70 TT=7.20n Vpk=50.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_B560C D ( IS=66.7u RS=14.1m BV=60.0 IBV=500u CJO=497p M=0.333 N=1.70 TT=7.20n Vpk=60.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT1000 D ( IS=874n RS=65.3m BV=40.0 IBV=100u CJO=175p M=0.333 N=0.823 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT400D D ( IS=1.80u RS=0.103 BV=40.0 IBV=50.0u CJO=119p M=0.333 N=1.26 TT=7.20n Vpk=40.0V Iave=0.500A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT750 D ( IS=23.1u RS=82.3m BV=40.0 IBV=100u CJO=225p M=0.333 N=1.16 TT=7.20n Vpk=40.0V Iave=0.750A mfg=DiodesInc type=Schottky )
.MODEL DI_BAT760 D ( IS=10.6u RS=49.9m BV=30.0 IBV=50.0u CJO=49.3p M=0.333 N=1.35 TT=14.4n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS1100 D ( IS=235n RS=27.5m BV=100 IBV=1.00u CJO=70.9p M=0.333 N=1.48 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS1150 D ( IS=10.2u RS=27.0m BV=150 IBV=2.00u CJO=55.2p M=0.333 N=2.32 TT=4.32u Vpk=150V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS120L D ( IS=21.0u RS=46.3m BV=20.0 IBV=1.00m CJO=252p M=0.333 N=0.936 TT=7.20n Vpk=20.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DFLS130 D ( IS=35.5u RS=54.5m BV=30.0 IBV=1.00m CJO=97.1p M=0.333 N=1.09 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DFLS130L D ( IS=7.74u RS=59.7m BV=30.0 IBV=1.00m CJO=225p M=0.333 N=0.832 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS140 D ( IS=163n RS=0.103 BV=40.0 IBV=20.0u CJO=99.4p M=0.333 N=1.00 TT=7.20n Vpk=40.0V Iave=1.10A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS140L D ( IS=817n RS=32.2m BV=40.0 IBV=500u CJO=293p M=0.333 N=1.01 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS160 D ( IS=736n RS=63.0m BV=60.0 IBV=100u CJO=163p M=0.333 N=1.01 TT=4.32u Vpk=60.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS220L D ( IS=20.3u RS=47.4m BV=20.0 IBV=1.00m CJO=252p M=0.333 N=0.947 TT=7.20n Vpk=20.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS230 D ( IS=100u RS=52.2m BV=30.0 IBV=1.00m CJO=133p M=0.333 N=1.27 TT=7.20n Vpk=30.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS230L D ( IS=125u RS=43.6m BV=30.0 IBV=1.00m CJO=265p M=0.333 N=1.21 TT=7.20n Vpk=30.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS230LH D ( IS=947n RS=32.4m BV=30.0 IBV=200u CJO=206p M=0.333 N=0.957 TT=15.8n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_DFLS240L D ( IS=516n RS=31.4m BV=40.0 IBV=500u CJO=292p M=0.333 N=0.911 TT=7.20n Vpk=40.0V Iave=2.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRB1530CT D ( IS=71.5u RS=2.81m BV=30.0 IBV=100u CJO=464p M=0.333 N=1.61 TT=43.2n Vpk=30.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRB1535CT D ( IS=71.5u RS=2.81m BV=35.0 IBV=100u CJO=464p M=0.333 N=1.61 TT=43.2n Vpk=35.0V Iave=15.0A mfg=DiodesInc type=silicon )
.MODEL DI_MBRB1540CT D ( IS=71.5u RS=2.81m BV=40.0 IBV=100u CJO=464p M=0.333 N=1.61 TT=43.2n Vpk=40.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRD1040 D ( IS=354u RS=4.20m BV=40.0 IBV=300u CJO=2.65n M=0.333 N=1.19 TT=7.20n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRD1040CT D ( IS=2.14m RS=6.38m BV=40.0 IBV=150u CJO=925p M=0.333 N=3.30 TT=14.4n Vpk=40.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRD835L D ( IS=9.28u RS=9.26m BV=35.0 IBV=1.40m CJO=1.11n M=0.333 N=1.06 TT=14.4n Vpk=35.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRM3100 D ( IS=88.1u RS=14.0m BV=100 IBV=100u CJO=239p M=0.333 N=2.12 TT=7.20n Vpk=100V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRM360 D ( IS=5.99u RS=16.5m BV=60.0 IBV=200u CJO=240p M=0.333 N=1.27 TT=14.4n Vpk=60.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBRM560 D ( IS=20.1u RS=8.40m BV=60.0 IBV=200u CJO=207p M=0.333 N=1.70 TT=7.20n Vpk=60.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS1040 D ( IS=2.78u RS=2.78m BV=40.0 IBV=700u CJO=1.72n M=0.333 N=1.05 TT=14.4n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL Di_PDS1040CTL D ( IS=21.5u RS=4.20m BV=40.0 IBV=200u CJO=789p M=0.333 N=1.28 TT=28.8n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL Di_PDS1040L D ( IS=6.02u RS=4.20m BV=40.0 IBV=600u CJO=2.21n M=0.333 N=1.04 TT=50.4n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS3100 D ( IS=20.9u RS=13.9m BV=100 IBV=200u CJO=305p M=0.333 N=1.70 TT=14.4n Vpk=100V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS3200 D ( IS=51.7u RS=11.3m BV=200 IBV=10.0u CJO=630p M=0.333 N=2.21 TT=14.4n Vpk=200V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS340 D ( IS=2.59u RS=13.5m BV=40.0 IBV=500u CJO=630p M=0.333 N=1.11 TT=18.7n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS5100 D ( IS=49.0u RS=7.63m BV=100 IBV=200u CJO=375p M=0.333 N=1.84 TT=21.6n Vpk=100V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS5100H D ( IS=1.32u RS=7.00m BV=100 IBV=10.0u CJO=676p M=0.333 N=1.37 TT=14.4n Vpk=100V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS540 D ( IS=9.59u RS=10.7m BV=40.0 IBV=300u CJO=727p M=0.333 N=1.26 TT=21.6n Vpk=40.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_PDS835L D ( IS=42.9u RS=6.30m BV=35.0 IBV=1.40m CJO=623p M=0.333 N=1.43 TT=21.6n Vpk=35.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1025L D ( IS=2.36u RS=7.72m BV=25.0 IBV=1.00m CJO=636p M=0.333 N=0.722 TT=7.20n Vpk=25.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1030CT D ( IS=759u RS=4.20m BV=30.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1030L D ( IS=2.36u RS=7.72m BV=30.0 IBV=1.00m CJO=636p M=0.333 N=0.722 TT=7.20n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1035CT D ( IS=759u RS=4.20m BV=35.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=35.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1040CT D ( IS=759u RS=4.20m BV=40.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1045CT D ( IS=759u RS=4.20m BV=45.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=45.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1630CT D ( IS=47.2u RS=6.69m BV=30.0 IBV=1.00m CJO=464p M=0.333 N=1.41 TT=7.20n Vpk=30.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1635CT D ( IS=47.2u RS=6.69m BV=35.0 IBV=1.00m CJO=464p M=0.333 N=1.41 TT=7.20n Vpk=35.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1640CT D ( IS=47.2u RS=6.69m BV=40.0 IBV=1.00m CJO=464p M=0.333 N=1.41 TT=7.20n Vpk=40.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG1645CT D ( IS=47.2u RS=6.69m BV=45.0 IBV=1.00m CJO=464p M=0.333 N=1.41 TT=7.20n Vpk=45.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG2030CT D ( IS=7.84m RS=3.91m BV=30.0 IBV=1.00m CJO=1.72n M=0.333 N=2.73 TT=7.20n Vpk=30.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG2035CT D ( IS=7.84m RS=3.91m BV=35.0 IBV=1.00m CJO=1.72n M=0.333 N=2.73 TT=7.20n Vpk=35.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG2040CT D ( IS=7.84m RS=3.91m BV=40.0 IBV=1.00m CJO=1.72n M=0.333 N=2.73 TT=7.20n Vpk=40.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG2045CT D ( IS=7.84m RS=3.91m BV=45.0 IBV=1.00m CJO=1.72n M=0.333 N=2.73 TT=7.20n Vpk=45.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG3030CT D ( IS=31.1u RS=3.70m BV=30.0 IBV=1.00m CJO=796p M=0.333 N=1.17 TT=7.20n Vpk=30.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG3040CT D ( IS=31.1u RS=3.70m BV=40.0 IBV=1.00m CJO=796p M=0.333 N=1.17 TT=7.20n Vpk=40.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG3045CT D ( IS=31.1u RS=3.70m BV=45.0 IBV=1.00m CJO=796p M=0.333 N=1.17 TT=7.20n Vpk=45.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG3050CT D ( IS=319u RS=3.50m BV=50.0 IBV=1.00m CJO=796p M=0.333 N=1.69 TT=7.20n Vpk=50.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBG3060CT D ( IS=319u RS=3.50m BV=60.0 IBV=1.00m CJO=796p M=0.333 N=1.69 TT=7.20n Vpk=60.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBM340 D ( IS=2.98n RS=19.4m BV=40.0 IBV=500u CJO=333p M=0.333 N=0.700 TT=14.4n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBM540 D ( IS=19.7u RS=8.40m BV=40.0 IBV=500u CJO=557p M=0.333 N=1.28 TT=14.4n Vpk=40.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_10A01 D ( IS=844n RS=2.06m BV=50.0 IBV=10.0u CJO=277p M=0.333 N=2.06 TT=4.32u Vpk=50.0V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A02 D ( IS=844n RS=2.06m BV=100 IBV=10.0u CJO=277p M=0.333 N=2.06 TT=4.32u Vpk=100V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A03 D ( IS=844n RS=2.06m BV=200 IBV=10.0u CJO=277p M=0.333 N=2.06 TT=4.32u Vpk=200V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A04 D ( IS=844n RS=2.06m BV=400 IBV=10.0u CJO=277p M=0.333 N=2.06 TT=4.32u Vpk=400V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A05 D ( IS=844n RS=2.06m BV=600 IBV=10.0u CJO=148p M=0.333 N=2.06 TT=4.32u Vpk=600V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A06 D ( IS=844n RS=2.06m BV=800 IBV=10.0u CJO=148p M=0.333 N=2.06 TT=4.32u Vpk=800V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_10A07 D ( IS=844n RS=2.06m BV=1.00k IBV=10.0u CJO=148p M=0.333 N=2.06 TT=4.32u Vpk=1.00kV Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_1N4001 D ( IS=76.9p RS=42.0m BV=50.0 IBV=5.00u CJO=39.8p M=0.333 N=1.45 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4001G D ( IS=65.4p RS=42.2m BV=50.0 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4001GL D ( IS=65.4p RS=42.2m BV=50.0 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4002 D ( IS=76.9p RS=42.0m BV=100 IBV=5.00u CJO=39.8p M=0.333 N=1.45 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4002G D ( IS=65.4p RS=42.2m BV=100 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4002GL D ( IS=65.4p RS=42.2m BV=100 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4003 D ( IS=76.9p RS=42.0m BV=200 IBV=5.00u CJO=39.8p M=0.333 N=1.45 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4003G D ( IS=65.4p RS=42.2m BV=200 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4003GL D ( IS=65.4p RS=42.2m BV=200 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4004 D ( IS=76.9p RS=42.0m BV=400 IBV=5.00u CJO=39.8p M=0.333 N=1.45 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4004G D ( IS=65.4p RS=42.2m BV=400 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4004GL D ( IS=65.4p RS=42.2m BV=400 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4005 D ( IS=76.9p RS=42.0m BV=600 IBV=5.00u CJO=26.5p M=0.333 N=1.45 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4005G D ( IS=65.4p RS=42.2m BV=600 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4005GL D ( IS=65.4p RS=42.2m BV=600 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4006 D ( IS=76.9p RS=42.0m BV=800 IBV=5.00u CJO=26.5p M=0.333 N=1.45 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4006G D ( IS=65.4p RS=42.2m BV=800 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4006GL D ( IS=65.4p RS=42.2m BV=800 IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4007 D ( IS=76.9p RS=42.0m BV=1.00k IBV=5.00u CJO=26.5p M=0.333 N=1.45 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4007G D ( IS=65.4p RS=42.2m BV=1.00k IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4007GL D ( IS=65.4p RS=42.2m BV=1.00k IBV=5.00u CJO=14.8p M=0.333 N=1.36 TT=2.88u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5400 D ( IS=63.0n RS=14.1m BV=50.0 IBV=10.0u CJO=125p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5401 D ( IS=63.0n RS=14.1m BV=100 IBV=10.0u CJO=125p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5402 D ( IS=63.0n RS=14.1m BV=200 IBV=10.0u CJO=125p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5404 D ( IS=63.0n RS=14.1m BV=400 IBV=10.0u CJO=125p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5406 D ( IS=63.0n RS=14.1m BV=600 IBV=10.0u CJO=53.0p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5407 D ( IS=63.0n RS=14.1m BV=800 IBV=10.0u CJO=53.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N5408 D ( IS=63.0n RS=14.1m BV=1.00k IBV=10.0u CJO=53.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A05 D ( IS=52.4n RS=7.00m BV=50.0 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=50.0V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A1 D ( IS=52.4n RS=7.00m BV=100 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=100V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A10 D ( IS=52.4n RS=7.00m BV=1.00k IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=1.00kV Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A2 D ( IS=52.4n RS=7.00m BV=200 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=200V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A4 D ( IS=52.4n RS=7.00m BV=400 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=400V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A6 D ( IS=52.4n RS=7.00m BV=600 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=600V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_6A8 D ( IS=52.4n RS=7.00m BV=800 IBV=10.0u CJO=60.0p M=0.333 N=1.70 TT=2.88u Vpk=800V Iave=6.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4001 D ( IS=7.96n RS=50.7m BV=50.0 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4002 D ( IS=7.96n RS=50.7m BV=100 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4003 D ( IS=7.96n RS=50.7m BV=200 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4004 D ( IS=7.96n RS=50.7m BV=400 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4005 D ( IS=7.96n RS=50.7m BV=600 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4006 D ( IS=7.96n RS=50.7m BV=800 IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_DL4007 D ( IS=7.96n RS=50.7m BV=1.00k IBV=5.00u CJO=27.7p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1A D ( IS=7.31e-018 RS=42.0m BV=50.0 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1AB D ( IS=7.31e-018 RS=42.0m BV=50.0 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=50.0V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1B D ( IS=7.31e-018 RS=42.0m BV=100 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1BB D ( IS=7.31e-018 RS=42.0m BV=100 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=100V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1D D ( IS=7.31e-018 RS=42.0m BV=200 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1DB D ( IS=7.31e-018 RS=42.0m BV=200 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=200V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1G D ( IS=7.31e-018 RS=42.0m BV=400 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1GB D ( IS=7.31e-018 RS=42.0m BV=400 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=400V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1J D ( IS=7.31e-018 RS=42.0m BV=600 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1JB D ( IS=7.31e-018 RS=42.0m BV=600 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=600V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1K D ( IS=7.31e-018 RS=42.0m BV=800 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1KB D ( IS=7.31e-018 RS=42.0m BV=800 IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=800V Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1M D ( IS=7.31e-018 RS=42.0m BV=1.00k IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S1MB D ( IS=7.31e-018 RS=42.0m BV=1.00k IBV=5.00u CJO=42.4p M=0.333 N=0.775 TT=4.32u Vpk=1.00kV Iave=1.00A mfg=DiodesInc type=silicon )
.MODEL DI_S2A D ( IS=1.30u RS=8.92m BV=50.0 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2AA D ( IS=1.30u RS=8.92m BV=50.0 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=50.0V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2B D ( IS=1.30u RS=8.92m BV=100 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2BA D ( IS=1.30u RS=8.92m BV=100 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=100V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2D D ( IS=1.30u RS=8.92m BV=200 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2DA D ( IS=1.30u RS=8.92m BV=200 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=200V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2G D ( IS=1.30u RS=8.92m BV=400 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2GA D ( IS=1.30u RS=8.92m BV=400 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=400V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2J D ( IS=1.30u RS=8.92m BV=600 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2JA D ( IS=1.30u RS=8.92m BV=600 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=600V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2K D ( IS=1.30u RS=8.92m BV=800 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2KA D ( IS=1.30u RS=8.92m BV=800 IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=800V Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2M D ( IS=1.30u RS=8.92m BV=1.00k IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S2MA D ( IS=1.30u RS=8.92m BV=1.00k IBV=5.00u CJO=37.0p M=0.333 N=2.58 TT=4.32u Vpk=1.00kV Iave=1.50A mfg=DiodesInc type=silicon )
.MODEL DI_S3A D ( IS=1.37n RS=14.0m BV=50.0 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=50.0V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3BB D ( IS=1.37n RS=14.0m BV=100 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=100V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3D D ( IS=1.37n RS=14.0m BV=200 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3DB D ( IS=1.37n RS=14.0m BV=200 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=200V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3GB D ( IS=1.37n RS=14.0m BV=400 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=400V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3K D ( IS=1.37n RS=14.0m BV=800 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=800V Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S3M D ( IS=1.37n RS=14.0m BV=1.00k IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=4.32u Vpk=1.00kV Iave=3.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5AC D ( IS=2.28n RS=8.40m BV=50.0 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=50.0V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5BC D ( IS=2.28n RS=8.40m BV=100 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=100V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5DC D ( IS=2.28n RS=8.40m BV=200 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=200V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5GC D ( IS=2.28n RS=8.40m BV=400 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=400V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5JC D ( IS=2.28n RS=8.40m BV=600 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=600V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5KC D ( IS=2.28n RS=8.40m BV=800 IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=800V Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_S5MC D ( IS=2.28n RS=8.40m BV=1.00k IBV=10.0u CJO=74.0p M=0.333 N=1.70 TT=2.88u Vpk=1.00kV Iave=5.00A mfg=DiodesInc type=silicon )
.MODEL DI_1N4148 D ( IS=222p RS=68.6m BV=75.0 IBV=1.00u CJO=4.00p M=0.333 N=1.65 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_1N4148W D ( IS=10.4n RS=51.5m BV=75.0 IBV=1.00u CJO=2.00p M=0.333 N=2.07 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_1N4148WS D ( IS=10.4n RS=51.5m BV=75.0 IBV=1.00u CJO=2.00p M=0.333 N=2.07 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_1N4148WT D ( IS=111n RS=0.628 BV=80.0 IBV=1.00u CJO=2.00p M=0.333 N=1.70 TT=5.76n Vpk=80.0V Iave=0.125A mfg=DiodesInc type=silicon )
.MODEL DI_1N4448HWS D ( IS=24.7n RS=84.4m BV=80.0 IBV=100n CJO=3.50p M=0.333 N=2.12 TT=5.76n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_1N4448HWT D ( IS=137f RS=0.168 BV=80.0 IBV=100n CJO=3.56p M=0.333 N=1.11 TT=5.76n Vpk=80.0V Iave=0.250A mfg=DiodesInc type=silicon )
.MODEL DI_1N4448W D ( IS=355p RS=0.168 BV=75.0 IBV=2.50u CJO=4.00p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.250A mfg=DiodesInc type=silicon )
.MODEL DI_1N4448WS D ( IS=24.7n RS=84.4m BV=75.0 IBV=2.50u CJO=4.00p M=0.333 N=2.12 TT=5.76n Vpk=75.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_BAL99 D ( IS=31.2n RS=0.360 BV=75.0 IBV=2.50u CJO=1.72p M=0.333 N=2.35 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAS116 D ( IS=4.53u RS=0.383 BV=60.0 IBV=5.00n CJO=1.72p M=0.333 N=4.07 TT=4.32u Vpk=60.0V Iave=0.215A mfg=DiodesInc type=silicon )
.MODEL DI_BAS116T D ( IS=10.5p RS=0.196 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.61 TT=4.32u Vpk=85.0V Iave=0.215A mfg=DiodesInc type=silicon )
.MODEL DI_BAS16T D ( IS=2.69n RS=0.271 BV=85.0 IBV=2.00u CJO=1.99p M=0.333 N=1.95 TT=5.76n
.MODEL DI_BAS16TW D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAS16V D ( IS=412p RS=0.140 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAS16W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAS19 D ( IS=41.7n RS=0.270 BV=100 IBV=100n CJO=2.98p M=0.333 N=2.35 TT=72.0n Vpk=100V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS19W D ( IS=114n RS=0.172 BV=100 IBV=100n CJO=2.98p M=0.333 N=2.58 TT=72.0n Vpk=100V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS20 D ( IS=41.7n RS=0.270 BV=150 IBV=100n CJO=2.98p M=0.333 N=2.35 TT=72.0n Vpk=150V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS20W D ( IS=114n RS=0.172 BV=150 IBV=100n CJO=2.98p M=0.333 N=2.58 TT=72.0n Vpk=150V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS21 D ( IS=41.7n RS=0.270 BV=200 IBV=100n CJO=2.98p M=0.333 N=2.35 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS21T D ( IS=401n RS=0.105 BV=200 IBV=100n CJO=5.00p M=0.333 N=2.87 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAS21W D ( IS=114n RS=0.172 BV=200 IBV=100n CJO=2.98p M=0.333 N=2.58 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV116W D ( IS=22.5p RS=0.282 BV=130 IBV=5.00n CJO=2.40p M=0.333 N=1.67 TT=4.32u Vpk=130V Iave=0.215A mfg=DiodesInc type=silicon )
.MODEL DI_BAV16W D ( IS=10.4n RS=51.5m BV=75.0 IBV=1.00u CJO=2.00p M=0.333 N=2.07 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV16WS D ( IS=10.4n RS=51.5m BV=75.0 IBV=1.00u CJO=2.00p M=0.333 N=2.07 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV170T D ( IS=10.5p RS=0.196 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.61 TT=4.32u Vpk=85.0V Iave=0.125A mfg=DiodesInc type=silicon )
.MODEL DI_BAV199 D ( IS=59.0p RS=0.262 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.78 TT=4.32u Vpk=85.0V Iave=0.160A mfg=DiodesInc type=silicon )
.MODEL DI_BAV199DW D ( IS=59.0p RS=0.262 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.78 TT=4.32u Vpk=85.0V Iave=0.160A mfg=DiodesInc type=silicon )
.MODEL DI_BAV199T D ( IS=10.5p RS=0.196 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.61 TT=4.32u Vpk=85.0V Iave=0.125A mfg=DiodesInc type=silicon )
.MODEL DI_BAV19W D ( IS=1.09u RS=0.105 BV=100 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=100V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV19WS D ( IS=1.09u RS=0.105 BV=100 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=100V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV20W D ( IS=1.09u RS=0.105 BV=150 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=150V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV20WS D ( IS=1.09u RS=0.105 BV=150 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=150V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV21W D ( IS=1.09u RS=0.105 BV=200 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV21WS D ( IS=1.09u RS=0.105 BV=200 IBV=100n CJO=5.00p M=0.333 N=3.29 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV23A D ( IS=237n RS=0.260 BV=200 IBV=100n CJO=3.05p M=0.333 N=2.69 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV23C D ( IS=237n RS=0.260 BV=200 IBV=100n CJO=3.05p M=0.333 N=2.69 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV23S D ( IS=237n RS=0.260 BV=200 IBV=100n CJO=3.05p M=0.333 N=2.69 TT=72.0n Vpk=200V Iave=0.400A mfg=DiodesInc type=silicon )
.MODEL DI_BAV3004W D ( IS=58.9n RS=0.412 BV=350 IBV=100n CJO=1.17p M=0.333 N=2.37 TT=72.0n Vpk=350V Iave=0.225A mfg=DiodesInc type=silicon )
.MODEL DI_BAV70 D ( IS=308p RS=0.329 BV=75.0 IBV=2.50u CJO=2.65p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV70T D ( IS=2.69n RS=0.271 BV=85.0 IBV=2.00u CJO=1.99p M=0.333 N=1.95 TT=5.76n Vpk=85.0V Iave=0.155A mfg=DiodesInc type=silicon )
.MODEL DI_BAV70W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV756DW D ( IS=49.2n RS=0.141 BV=75.0 IBV=2.50u CJO=2.65p M=0.333 N=2.45 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV99 D ( IS=261p RS=0.140 BV=75.0 IBV=2.50u CJO=1.19p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV99BRW D ( IS=412p RS=0.140 BV=75.0 IBV=2.50u CJO=2.00p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV99DW D ( IS=412p RS=0.140 BV=75.0 IBV=2.50u CJO=2.00p M=0.333 N=1.70 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAV99T D ( IS=2.69n RS=0.271 BV=85.0 IBV=2.00u CJO=1.99p M=0.333 N=1.95 TT=5.76n Vpk=85.0V Iave=0.155A mfg=DiodesInc type=silicon )
.MODEL DI_BAV99W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAW156 D ( IS=59.0p RS=0.262 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.78 TT=4.32u Vpk=85.0V Iave=0.160A mfg=DiodesInc type=silicon )
.MODEL DI_BAW156T D ( IS=10.5p RS=0.196 BV=85.0 IBV=5.00n CJO=2.00p M=0.333 N=1.61 TT=4.32u Vpk=85.0V Iave=0.125A mfg=DiodesInc type=silicon )
.MODEL DI_BAW56 D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAW567DW D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAW56DW D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_BAW56T D ( IS=2.69n RS=0.271 BV=85.0 IBV=2.00u CJO=1.99p M=0.333 N=1.95 TT=5.76n Vpk=85.0V Iave=0.155A mfg=DiodesInc type=silicon )
.MODEL DI_BAW56W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD2004S D ( IS=1.76u RS=0.187 BV=240 IBV=100n CJO=6.63p M=0.333 N=1.70 TT=72.0n Vpk=240V Iave=0.225A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD2004SW D ( IS=1.76u RS=0.187 BV=240 IBV=100n CJO=6.63p M=0.333 N=1.70 TT=72.0n Vpk=240V Iave=0.225A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD3004BRM D ( IS=2.76u RS=0.187 BV=300 IBV=100n CJO=1.17p M=0.333 N=1.70 TT=72.0n Vpk=300V Iave=0.225A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD3004S D ( IS=2.76u RS=0.187 BV=300 IBV=100n CJO=1.17p M=0.333 N=1.70 TT=72.0n Vpk=300V Iave=0.225A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4148_1 D ( IS=126n RS=0.140 BV=75.0 IBV=1.00u CJO=2.65p M=0.333 N=2.60 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4148 D ( IS=300n RS=0.422 BV=75.0 IBV=2.50u CJO=1.99p M=0.333 N=2.77 TT=5.76n Vpk=75.0V Iave=0.250A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4148W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448 D ( IS=300n RS=0.422 BV=75.0 IBV=2.50u CJO=1.99p M=0.333 N=2.77 TT=5.76n Vpk=75.0V Iave=0.250A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448H D ( IS=300n RS=0.422 BV=80.0 IBV=100n CJO=1.99p M=0.333 N=2.77 TT=5.76n Vpk=80.0V Iave=0.250A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HADW D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HAQW D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HCQW D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HSDW D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HT D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HTA D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HTC D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HTS D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HTW D ( IS=1.12n RS=84.0m BV=80.0 IBV=100n CJO=2.92p M=0.333 N=1.70 TT=2.16n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448HW D ( IS=77.0n RS=84.0m BV=80.0 IBV=100n CJO=1.99p M=0.333 N=2.37 TT=5.76n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448V D ( IS=4.77n RS=84.4m BV=80.0 IBV=100n CJO=1.99p M=0.333 N=1.95 TT=5.76n Vpk=80.0V Iave=0.500A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD4448W D ( IS=68.6n RS=0.377 BV=75.0 IBV=1.00u CJO=1.72p M=0.333 N=2.34 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD7000 D ( IS=5.08n RS=0.140 BV=75.0 IBV=2.00u CJO=2.00p M=0.333 N=2.03 TT=5.76u Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_MMBD914 D ( IS=126n RS=0.140 BV=75.0 IBV=1.00u CJO=2.65p M=0.333 N=2.60 TT=5.76n Vpk=75.0V Iave=0.300A mfg=DiodesInc type=silicon )
.MODEL DI_1N5817 D ( IS=870u RS=81.3m BV=20.0 IBV=1.00m CJO=203p M=0.333 N=1.81 TT=4.32u Vpk=20.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_1N5818 D ( IS=263u RS=73.1m BV=30.0 IBV=1.00m CJO=203p M=0.333 N=1.90 TT=4.32u Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_1N5819 D ( IS=390n RS=0.115 BV=40.0 IBV=1.00m CJO=203p M=0.333 N=1.70 TT=4.32u Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR10100CT D ( IS=27.9n RS=4.20m BV=100 IBV=100u CJO=555p M=0.333 N=1.28 TT=7.20n Vpk=100V Iave=10.0A mfg=DiodesInc type=silicon )
.MODEL DI_MBR1030 D ( IS=2.62m RS=4.20m BV=30.0 IBV=100u CJO=796p M=0.333 N=2.12 TT=7.20n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1030CT D ( IS=4.25u RS=13.0m BV=30.0 IBV=100u CJO=318p M=0.333 N=1.15 TT=14.4n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1035 D ( IS=2.62m RS=4.20m BV=35.0 IBV=100u CJO=796p M=0.333 N=2.12 TT=7.20n Vpk=35.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1040 D ( IS=2.62m RS=4.20m BV=40.0 IBV=100u CJO=796p M=0.333 N=2.12 TT=7.20n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1040CT D ( IS=4.25u RS=13.0m BV=40.0 IBV=100u CJO=318p M=0.333 N=1.15 TT=14.4n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1045 D ( IS=2.62m RS=4.20m BV=45.0 IBV=100u CJO=796p M=0.333 N=2.12 TT=7.20n Vpk=45.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1045CT D ( IS=4.25u RS=13.0m BV=45.0 IBV=100u CJO=318p M=0.333 N=1.15 TT=14.4n Vpk=45.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1050 D ( IS=153u RS=3.17m BV=50.0 IBV=100u CJO=796p M=0.333 N=1.96 TT=7.20n Vpk=50.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1050CT D ( IS=7.24u RS=14.5m BV=50.0 IBV=100u CJO=318p M=0.333 N=1.29 TT=14.4n Vpk=50.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1060 D ( IS=153u RS=3.17m BV=60.0 IBV=100u CJO=796p M=0.333 N=1.96 TT=7.20n Vpk=60.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1060CT D ( IS=7.24u RS=14.5m BV=60.0 IBV=100u CJO=318p M=0.333 N=1.29 TT=14.4n Vpk=60.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1530CT D ( IS=344u RS=2.81m BV=30.0 IBV=25.0u CJO=530p M=0.333 N=2.28 TT=7.20n Vpk=30.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1535CT D ( IS=344u RS=2.81m BV=35.0 IBV=25.0u CJO=530p M=0.333 N=2.28 TT=7.20n Vpk=35.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1540CT D ( IS=344u RS=2.81m BV=40.0 IBV=25.0u CJO=530p M=0.333 N=2.28 TT=7.20n Vpk=40.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1545CT D ( IS=344u RS=2.81m BV=45.0 IBV=25.0u CJO=530p M=0.333 N=2.28 TT=7.20n Vpk=45.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1550CT D ( IS=11.3u RS=2.64m BV=50.0 IBV=25.0u CJO=530p M=0.333 N=1.87 TT=7.20n Vpk=50.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1560CT D ( IS=11.3u RS=2.64m BV=60.0 IBV=25.0u CJO=530p M=0.333 N=1.87 TT=7.20n Vpk=60.0V Iave=15.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1630 D ( IS=138u RS=2.62m BV=30.0 IBV=31.0u CJO=862p M=0.333 N=1.53 TT=7.20n Vpk=30.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1635 D ( IS=138u RS=2.62m BV=35.0 IBV=31.0u CJO=862p M=0.333 N=1.53 TT=7.20n Vpk=35.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1640 D ( IS=138u RS=2.62m BV=40.0 IBV=31.0u CJO=862p M=0.333 N=1.53 TT=7.20n Vpk=40.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1645 D ( IS=138u RS=2.62m BV=45.0 IBV=31.0u CJO=862p M=0.333 N=1.53 TT=7.20n Vpk=45.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1650 D ( IS=245u RS=1.99m BV=50.0 IBV=31.0u CJO=862p M=0.333 N=1.96 TT=7.20n Vpk=50.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR1660 D ( IS=245u RS=1.99m BV=60.0 IBV=31.0u CJO=862p M=0.333 N=1.96 TT=7.20n Vpk=60.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2030CT D ( IS=99.0u RS=2.10m BV=30.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=30.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2035CT D ( IS=98.9u RS=2.11m BV=35.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=35.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2040CT D ( IS=98.9u RS=2.11m BV=40.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=40.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2045CT D ( IS=98.9u RS=2.11m BV=45.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=45.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2050CT D ( IS=16.0u RS=2.11m BV=50.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=50.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2060CT D ( IS=16.0u RS=2.11m BV=60.0 IBV=60.0u CJO=994p M=0.333 N=1.70 TT=1.44n Vpk=60.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2535CT D ( IS=533u RS=1.41m BV=35.0 IBV=50.0u CJO=1.34n M=0.333 N=1.95 TT=1.44n Vpk=35.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2545CT D ( IS=533u RS=1.41m BV=45.0 IBV=50.0u CJO=1.34n M=0.333 N=1.95 TT=1.44n Vpk=45.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2550CT D ( IS=1.16m RS=1.41m BV=50.0 IBV=50.0u CJO=1.34k M=0.333 N=2.53 TT=1.44n Vpk=50.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_MBR2560CT D ( IS=1.16m RS=1.41m BV=60.0 IBV=50.0u CJO=1.34k M=0.333 N=2.53 TT=1.44n Vpk=60.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SB1100 D ( IS=6.63u RS=62.3m BV=100.0 IBV=500u CJO=199p M=0.333 N=1.70 TT=7.20n Vpk=100.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB120 D ( IS=31.5u RS=49.2m BV=20.0 IBV=500u CJO=239p M=0.333 N=1.70 TT=7.20n Vpk=20.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB130 D ( IS=31.5u RS=49.2m BV=30.0 IBV=500u CJO=239p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB140 D ( IS=31.5u RS=49.2m BV=40.0 IBV=500u CJO=239p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB150 D ( IS=1.17u RS=42.0m BV=50.0 IBV=500u CJO=172p M=0.333 N=1.28 TT=7.20n Vpk=50.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB160 D ( IS=1.17u RS=42.0m BV=60.0 IBV=500u CJO=172p M=0.333 N=1.28 TT=7.20n Vpk=60.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB170 D ( IS=6.63u RS=62.3m BV=70.0 IBV=500u CJO=199p M=0.333 N=1.70 TT=7.20n Vpk=70.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB180 D ( IS=6.63u RS=62.3m BV=80.0 IBV=500u CJO=199p M=0.333 N=1.70 TT=7.20n Vpk=80.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB190 D ( IS=6.63u RS=62.3m BV=90.0 IBV=500u CJO=199p M=0.333 N=1.70 TT=7.20n Vpk=90.0V Iave=1.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SB340 D ( IS=85.9n RS=18.5m BV=40.0 IBV=70.0u CJO=411p M=0.333 N=0.754 TT=7.20n Vpk=40.0V Iave=3.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1030 D ( IS=759u RS=4.20m BV=30.0 IBV=1.00m CJO=2.12n M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1030CT D ( IS=759u RS=4.20m BV=30.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1035 D ( IS=759u RS=4.20m BV=35.0 IBV=1.00m CJO=2.12n M=0.333 N=1.70 TT=7.20n Vpk=35.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1035CT D ( IS=759u RS=4.20m BV=35.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=35.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1040 D ( IS=759u RS=4.20m BV=40.0 IBV=1.00m CJO=2.12n M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1040CT D ( IS=759u RS=4.20m BV=40.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1045 D ( IS=759u RS=4.20m BV=45.0 IBV=1.00m CJO=2.12n M=0.333 N=1.70 TT=7.20n Vpk=45.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1045CT D ( IS=759u RS=4.20m BV=45.0 IBV=500u CJO=941p M=0.333 N=1.70 TT=7.20n Vpk=45.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1050 D ( IS=210u RS=4.22m BV=50.0 IBV=1.00m CJO=2.12n M=0.333 N=2.03 TT=7.20n Vpk=50.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1050CT D ( IS=210u RS=4.22m BV=50.0 IBV=500u CJO=941p M=0.333 N=2.03 TT=7.20n Vpk=50.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1060 D ( IS=210u RS=4.22m BV=60.0 IBV=1.00m CJO=2.12n M=0.333 N=2.03 TT=7.20n Vpk=60.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1060CT D ( IS=210u RS=4.22m BV=60.0 IBV=500u CJO=941p M=0.333 N=2.03 TT=7.20n Vpk=60.0V Iave=10.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1630 D ( IS=903u RS=3.60m BV=30.0 IBV=1.00m CJO=1.72n M=0.333 N=1.67 TT=7.20n Vpk=30.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1630PT D ( IS=575u RS=3.47m BV=30.0 IBV=500u CJO=1.86n M=0.333 N=1.68 TT=7.20n Vpk=30.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1635 D ( IS=903u RS=3.60m BV=35.0 IBV=1.00m CJO=1.72n M=0.333 N=1.67 TT=7.20n Vpk=35.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1635PT D ( IS=575u RS=3.47m BV=35.0 IBV=500u CJO=1.86n M=0.333 N=1.68 TT=7.20n Vpk=35.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1640 D ( IS=903u RS=3.60m BV=40.0 IBV=1.00m CJO=1.72n M=0.333 N=1.67 TT=7.20n Vpk=40.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1640PT D ( IS=575u RS=3.47m BV=40.0 IBV=500u CJO=1.86n M=0.333 N=1.68 TT=7.20n Vpk=40.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1645 D ( IS=903u RS=3.60m BV=45.0 IBV=1.00m CJO=1.72n M=0.333 N=1.67 TT=7.20n Vpk=45.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1645PT D ( IS=575u RS=3.47m BV=45.0 IBV=500u CJO=1.86n M=0.333 N=1.68 TT=7.20n Vpk=45.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1650 D ( IS=1.38m RS=3.22m BV=50.0 IBV=1.00m CJO=1.72n M=0.333 N=2.27 TT=7.20n Vpk=50.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1650PT D ( IS=89.9u RS=3.60m BV=50.0 IBV=500u CJO=1.86n M=0.333 N=1.67 TT=7.20n Vpk=50.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1660 D ( IS=1.38m RS=3.22m BV=60.0 IBV=1.00m CJO=1.72n M=0.333 N=2.27 TT=7.20n Vpk=60.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL1660PT D ( IS=89.9u RS=3.60m BV=60.0 IBV=500u CJO=1.86n M=0.333 N=1.67 TT=7.20n Vpk=60.0V Iave=16.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2030CT D ( IS=4.83m RS=2.37m BV=30.0 IBV=1.00m CJO=1.34n M=0.333 N=2.28 TT=14.4n Vpk=30.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2030PT D ( IS=597u RS=2.88m BV=30.0 IBV=1.00m CJO=2.52n M=0.333 N=1.59 TT=14.4n Vpk=30.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2035CT D ( IS=4.83m RS=2.37m BV=35.0 IBV=1.00m CJO=1.34n M=0.333 N=2.28 TT=14.4n Vpk=35.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2035PT D ( IS=597u RS=2.88m BV=35.0 IBV=1.00m CJO=2.52n M=0.333 N=1.59 TT=14.4n Vpk=35.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2040CT D ( IS=4.83m RS=2.37m BV=40.0 IBV=1.00m CJO=1.34n M=0.333 N=2.28 TT=14.4n Vpk=40.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2040PT D ( IS=597u RS=2.88m BV=40.0 IBV=1.00m CJO=2.52n M=0.333 N=1.59 TT=14.4n Vpk=40.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2045CT D ( IS=4.83m RS=2.37m BV=45.0 IBV=1.00m CJO=1.34n M=0.333 N=2.28 TT=14.4n Vpk=45.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2045PT D ( IS=597u RS=2.88m BV=45.0 IBV=1.00m CJO=2.52n M=0.333 N=1.59 TT=14.4n Vpk=45.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2050CT D ( IS=3.50m RS=2.11m BV=50.0 IBV=1.00m CJO=1.34n M=0.333 N=2.95 TT=14.4n Vpk=50.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2050PT D ( IS=587u RS=2.11m BV=50.0 IBV=1.00m CJO=2.52n M=0.333 N=2.12 TT=14.4n Vpk=50.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2060CT D ( IS=3.50m RS=2.11m BV=60.0 IBV=1.00m CJO=1.34n M=0.333 N=2.95 TT=14.4n Vpk=60.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL2060PT D ( IS=587u RS=2.11m BV=60.0 IBV=1.00m CJO=2.52n M=0.333 N=2.12 TT=14.4n Vpk=60.0V Iave=20.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3030CT D ( IS=200u RS=1.92m BV=30.0 IBV=1.00m CJO=809p M=0.333 N=1.42 TT=14.4n Vpk=30.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3030PT D ( IS=441u RS=1.92m BV=30.0 IBV=1.00m CJO=1.33n M=0.333 N=1.51 TT=14.4n Vpk=30.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3035PT D ( IS=441u RS=1.92m BV=35.0 IBV=1.00m CJO=1.33n M=0.333 N=1.51 TT=14.4n Vpk=35.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3040CT D ( IS=200u RS=1.92m BV=40.0 IBV=1.00m CJO=809p M=0.333 N=1.42 TT=14.4n Vpk=40.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3040PT D ( IS=441u RS=1.92m BV=40.0 IBV=1.00m CJO=1.33n M=0.333 N=1.51 TT=14.4n Vpk=40.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3045PT D ( IS=441u RS=1.92m BV=45.0 IBV=1.00m CJO=1.33n M=0.333 N=1.51 TT=14.4n Vpk=45.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3050PT D ( IS=346u RS=1.61m BV=50.0 IBV=1.00m CJO=1.33n M=0.333 N=2.02 TT=14.4n Vpk=50.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL3060PT D ( IS=346u RS=1.61m BV=60.0 IBV=1.00m CJO=1.33n M=0.333 N=2.02 TT=14.4n Vpk=60.0V Iave=30.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4030PT D ( IS=10.9u RS=1.53m BV=30.0 IBV=1.00m CJO=1.33n M=0.333 N=1.08 TT=14.4n Vpk=30.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4035PT D ( IS=10.9u RS=1.53m BV=35.0 IBV=1.00m CJO=1.33n M=0.333 N=1.08 TT=14.4n Vpk=35.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4040PT D ( IS=10.9u RS=1.53m BV=40.0 IBV=1.00m CJO=1.33n M=0.333 N=1.08 TT=14.4n Vpk=40.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4045PT D ( IS=10.9u RS=1.53m BV=45.0 IBV=1.00m CJO=1.33n M=0.333 N=1.08 TT=14.4n Vpk=45.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4050PT D ( IS=53.0u RS=1.26m BV=50.0 IBV=1.00m CJO=1.33n M=0.333 N=1.70 TT=14.4n Vpk=50.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL4060PT D ( IS=53.0u RS=1.26m BV=60.0 IBV=1.00m CJO=1.33n M=0.333 N=1.70 TT=14.4n Vpk=60.0V Iave=40.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL530 D ( IS=926u RS=9.47m BV=30.0 IBV=500u CJO=968p M=0.333 N=1.69 TT=14.4n Vpk=30.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL535 D ( IS=926u RS=9.47m BV=35.0 IBV=500u CJO=968p M=0.333 N=1.69 TT=14.4n Vpk=35.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL540 D ( IS=926u RS=9.47m BV=40.0 IBV=500u CJO=968p M=0.333 N=1.69 TT=14.4n Vpk=40.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL545 D ( IS=926u RS=9.47m BV=45.0 IBV=500u CJO=968p M=0.333 N=1.69 TT=14.4n Vpk=45.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL550 D ( IS=14.0u RS=8.33m BV=50.0 IBV=500u CJO=968p M=0.333 N=1.70 TT=14.4n Vpk=50.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL560 D ( IS=14.0u RS=8.33m BV=60.0 IBV=500u CJO=968p M=0.333 N=1.70 TT=14.4n Vpk=60.0V Iave=5.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL6030PT D ( IS=1.93m RS=917u BV=30.0 IBV=20.0m CJO=3.25n M=0.333 N=1.68 TT=14.4n Vpk=30.0V Iave=60.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL6040PT D ( IS=1.93m RS=917u BV=40.0 IBV=20.0m CJO=3.25n M=0.333 N=1.68 TT=14.4n Vpk=40.0V Iave=60.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL6050PT D ( IS=353u RS=909u BV=50.0 IBV=20.0m CJO=3.25n M=0.333 N=1.76 TT=14.4n Vpk=50.0V Iave=60.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL6060PT D ( IS=353u RS=909u BV=60.0 IBV=20.0m CJO=3.25n M=0.333 N=1.76 TT=14.4n Vpk=60.0V Iave=60.0A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL830 D ( IS=396u RS=4.50m BV=30.0 IBV=500u CJO=1.72n M=0.333 N=1.71 TT=14.4n Vpk=30.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL835 D ( IS=396u RS=4.50m BV=35.0 IBV=500u CJO=1.72n M=0.333 N=1.71 TT=14.4n Vpk=35.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL840 D ( IS=396u RS=4.50m BV=40.0 IBV=500u CJO=1.72n M=0.333 N=1.71 TT=14.4n Vpk=40.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL845 D ( IS=396u RS=4.50m BV=45.0 IBV=500u CJO=1.72n M=0.333 N=1.71 TT=14.4n Vpk=45.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL850 D ( IS=30.8u RS=5.66m BV=50.0 IBV=500u CJO=1.72n M=0.333 N=1.69 TT=14.4n Vpk=50.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SBL860 D ( IS=30.8u RS=5.66m BV=60.0 IBV=500u CJO=1.72n M=0.333 N=1.69 TT=14.4n Vpk=60.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SD830 D ( IS=248u RS=5.25m BV=30.0 IBV=1.00m CJO=1.06n M=0.333 N=1.70 TT=7.20n Vpk=30.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SD840 D ( IS=248u RS=5.25m BV=40.0 IBV=1.00m CJO=1.06n M=0.333 N=1.70 TT=7.20n Vpk=40.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SD845 D ( IS=248u RS=5.25m BV=45.0 IBV=1.00m CJO=1.06n M=0.333 N=1.70 TT=7.20n Vpk=45.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DI_SD860 D ( IS=248u RS=5.25m BV=60.0 IBV=1.00m CJO=1.06n M=0.333 N=1.70 TT=7.20n Vpk=60.0V Iave=8.00A mfg=DiodesInc type=Schottky )
.MODEL DSEP8-12A D(IS=3.7288E-6 N=4.9950 RS=72.502E-3 IKF=999 CJO=1.0000E-12 M=.3333 VJ=.75 ISR=4.8113E-6 BV=1.2002E3 IBV=21.554E-3 TT=31.929E-9 mfg=IXYS type=silicon Vpk=1200.0V Iave=8.0A)
.MODEL DSEP29-12A D(IS=2.6918E-6 N=4.9950 RS=18.105E-3 IKF=999 CJO=1.0000E-12 M=.3333 VJ=.75 ISR=21.145E-6 BV=1.2001E3 IBV=2.1553E-3 TT=16.681E-9 mfg=IXYS type=silicon Vpk=1200.0V Iave=29.0A)
.MODEL DSEI60-06A D( IS=148.21E-6 N=1.8882 RS=3.0622E-3 IKF=811.78E-9 CJO=1.0000E-12 M=.3333 VJ=.75 ISR=406.73E-9 NR=4.9950 BV=600.05 IBV=1.2932E-3 TT=26.602E-9 Vpk=600 Iave=60A mfg=IXYS type=silicon Vpk=600.0V Iave=60.0A)
.model MUR460-GI D(Is=149n Rs=0.0384 N=2 EG=1.285 XTI=0.5 BV=800 IBV=1e-05 Cjo=126.4p Vj=1.34 M=0.52 TT=44.4n Iave=4.0A Vpk=600.0V mfg=GI type=silicon)
.model MUR460-M D(Is=289.1f Rs=33.23m Ikf=5.678m N=1 Xti=5 Eg=1.11 Cjo=70.72p M=.5733 Vj=.75 Fc=.5 Isr=6.495n Nr=2 Tt=123.3n Iave=4.0A Vpk=600.0V mfg=Motorola type=silicon)
.model MUR160-M D(Is=1.043p Rs=74.44m Ikf=2.705m N=1 Xti=2 Eg=1.11 Cjo=28.43p M=.6225 Vj=.75 Fc=.5 Isr=7.011n Nr=2 Tt=123.3n Iave=1.0A Vpk=600.0V mfg=Motorola type=silicon)
.MODEL CSD06060 D(IS=479.17E-6 RS=70.317E-3 N=4.9950 CJO=537.33E-12 M=.40753 BV=800.13 IKF=1.0000E3 VJ=.3905 ISR=10.010E-21 NR=4.9950 IBV=.12937 TT=15.628E-12 Iave=6A Vpk=600V mfg=Cree type=Schottky)
***** PHILIPS *****
.MODEL PH_1N4735A D ( IS = 1.803E-14 N = 1.167 BV = 6.2 IBV = 0.041 RS = 0.3264 CJO = 6.85E-11 VJ = 0.6947 M = 0.3439 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_1PS181 D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 EG = 1.1 XTI = 3 mfg=Philips type=silicon )
.MODEL PH_1PS300 D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 EG = 1.1 XTI = 3 mfg=Philips type=silicon )
.MODEL PH_BAS116 D ( IS=805.84E-18 N=1.0246 RS=50.000E-3 IKF=362.16E-6 CJO=1.9002E-12 M=.35193 VJ=1.2722 ISR=298.95E-15 BV=113.30 IBV=10 TT=1.0230E-6 mfg=Philips type=silicon )
.MODEL PH_BAS116H D ( IS=805.84E-18 N=1.0246 RS=50.000E-3 IKF=362.16E-6 CJO=1.9002E-12 M=.35193 VJ=1.2722 ISR=298.95E-15 BV=98 IBV=1.42E-3 TT=1.0230E-6 mfg=Philips type=silicon )
.MODEL PH_BAS16 D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646e-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS16H D( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646e-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9) mfg=Philips type=silicon )
.MODEL PH_BAS16L D ( IS = 6.0289E-9 N = 2.1283 RS = 1.0000E-3 IKF = 37.638E-3 CJO = 5.641E-013 M = 0.05188 VJ = 0.01571 ISR = 2.0646e-9 NR = 4.9950 BV = 113.60 IBV = 10 TT = 4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS16VV D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646e-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS16VY D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646e-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS21 D ( IS = 3.648E-9 N = 1.909 BV = 260 IBV = 2E-7 RS = 0.7535 CJO = 6.99E-13 VJ = 0.2028 M = 0.1151 FC = 0.5 TT = 3.462E-8 mfg=Philips type=silicon )
.MODEL PH_BAS216 D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646E-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS21H D ( IS = 3.648E-9 N = 1.909 BV = 260 IBV = 2E-7 RS = 0.7535 CJO = 6.99E-13 VJ = 0.2028 M = 0.1151 FC = 0.5 TT = 3.462E-8 mfg=Philips type=silicon )
.MODEL PH_BAS21VD D ( IS = 3.648E-9 N = 1.909 BV = 260 IBV = 2E-7 RS = 0.7535 CJO = 5.01E-13 VJ = 0.4515 M = 0.0571 FC = 0.5 TT = 2.054E-8 mfg=Philips type=silicon )
.MODEL PH_BAS28 D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646E-9 NR=4.9950 BV=113.60 IBV=10 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_BAS321 D ( IS=3.7106E-9 N=1.9403 RS=.41967 IKF=62.731E-3 CJO=412.54E-12 M=.1 VJ=2.2836 ISR=7.2305E-9 BV=319.86 IBV=5.1728E-6 TT=37.510E-9 mfg=Philips type=silicon )
.MODEL PH_BAS32L D ( IS=22.270E-9 N=2.2030 RS=1.0000E-3 IKF=16.940E-3 CJO=1.0350E-12 M=.1 VJ=.75 ISR=10.010E-21 BV=124.10 IBV=7.6070E-3 TT=4.3280E-9 mfg=Philips type=silicon )
.MODEL PH_BAS416 D ( IS=805.84E-18 N=1.0246 RS=50.000E-3 IKF=362.16E-6 CJO=1.9002E-12 M=.35193 VJ=1.2722 ISR=298.95E-15 BV=98 IBV=1.42E-3 TT=1.0230E-6 mfg=Philips type=silicon )
.MODEL PH_BAS45A D ( IS=7.0000E-9 N=2.2707 RS=1.0000E-3 IKF=22.121 CJO=2.9332E-12 M=.24677 VJ=.3905 ISR=10.010E-21 NR=4.9950 BV=225.36 IBV=10 TT=1.7500E-6 mfg=Philips type=silicon )
.MODEL PH_BAS516 D ( IS=2.9891E-9 N=1.9303 RS=0.78115 IKF=0.085491E-3 CJO=383.41E-15 M=.1 VJ=9.99 ISR=6.8038E-9 NR=4.9950 BV=130.38 IBV=10 TT=3.0297E-9 mfg=Philips type=silicon )
.MODEL PH_BAS521 D ( IS = 7.219E-9 N = 2 BV = 310 IBV = 0.0001 RS = 0.63 CJO = 4.074E-13 VJ = 0.6538 M = 0.05409 FC = 0.5 TT = 2.1987E-8 EG = 0.69 XTI = 2 mfg=Philips type=silicon )
.MODEL PH_BAS56 D ( IS=10.825E-9 N=1.9301 RS=.49924 IKF=1.4135 CJO=994.44E-15 M=.10001 VJ=.69196 ISR=1.0704E-9 BV=113.15 IBV=15.676E-3 TT=5.7708E-9 mfg=Philips type=silicon )
.MODEL PH_BAS716 D ( IS = 3.519E-15 N = 1.093 BV = 110 IBV = 3E-9 RS = 0.7423 CJO = 1.817E-12 VJ = 0.6508 M = 0.3689 FC = 0.5 TT = 8.656E-7 mfg=Philips type=silicon )
.MODEL PH_BAV103 D ( IS=21.910E-9 N=2.2330 RS=1.0000E-3 IKF=19.230E-3 CJO=1.0300E-12 M=.1001 VJ=.75 ISR=10.010E-21 BV=293.10 IBV=1.2930E-3 TT=51.940E-9 mfg=Philips type=silicon )
.MODEL PH_BAV199 D ( IS=805.84E-18 N=1.0246 RS=50.000E-3 IKF=362.16E-6 CJO=1.9002E-12 M=.35193 VJ=1.2722 ISR=298.95E-15 BV=113.30 IBV=10 TT=1.0230E-6 mfg=Philips type=silicon )
.MODEL PH_BAV23 D ( IS = 3.648E-9 N = 1.909 BV = 260 IBV = 2E-7 RS = 0.7535 CJO = 7.528E-13 VJ = 0.1936 M = 0.1285 FC = 0.5 TT = 3.462E-8 mfg=Philips type=silicon )
.MODEL PH_BAV23S D ( IS = 3.648E-9 N = 1.909 BV = 260 IBV = 2E-7 RS = 0.7535 CJO = 7.501E-13 VJ = 0.1995 M = 0.115 FC = 0.5 TT = 3.462E-8 mfg=Philips type=silicon )
.MODEL PH_BAV99S D ( IS=7.4960E-9 N=2.0077 RS=.80464 IKF=.1058 CJO=515.09E-15 M=.115 VJ=.6389 ISR=1.4182E-9 NR=4.9950 BV=90.375 IBV=10 TT=2.1640E-9 mfg=Philips type=silicon )
.MODEL PH_BAW101 D ( IS = 7.219E-9 N = 2 BV = 310 IBV = 0.0001 RS = 0.63 CJO = 4.584E-13 VJ = 0.7483 M = 0.06257 FC = 0.5 TT = 2.1987E-8 mfg=Philips type=silicon )
.MODEL PH_BAW101S D ( IS = 7.219E-9 N = 2 BV = 310 IBV = 0.0001 RS = 0.63 CJO = 4.584E-13 VJ = 0.7483 M = 0.06257 FC = 0.5 TT = 2.1987E-8 mfg=Philips type=silicon )
.MODEL PH_BAW56 D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 mfg=Philips type=silicon )
.MODEL PH_BAW56S D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 EG = 1.1 XTI = 3 mfg=Philips type=silicon )
.MODEL PH_BAW56T D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 EG = 1.1 XTI = 3 mfg=Philips type=silicon )
.MODEL PH_BAW56W D ( IS = 1.705E-9 N = 1.71 BV = 87 IBV = 0.0003 RS = 1.022 CJO = 1.798E-12 VJ = 1.032 M = 0.2987 FC = 0.5 TT = 3.606E-9 EG = 1.1 XTI = 3 mfg=Philips type=silicon )
.MODEL PH_BAW62 D ( IS = 3.126E-9 N = 1.925 BV = 85 IBV = 0.0005 RS = 0.8109 CJO = 7.27E-13 VJ = 0.7226 M = 0.01318 FC = 0.5 TT = 4.04E-9 mfg=Philips type=silicon )
.MODEL PH_BZA418A D ( IS = 2.26E-14 N = 1.135 BV = 17.9 IBV = 1E-09 RS = 0.2056 CJO = 4.079E-11 VJ = 0.5582 M = 0.381 FC = 0.5 TT = 7.502E-07 mfg=Philips type=zener )
.MODEL PH_BZA820A D ( IS=323.81E-18 N=.97963 RS=.24264 IKF=6.9002 CJO=37.279E-12 M=.32559 VJ=.3905 ISR=2.7811E-9 NR=2.4186 BV=19.919 IBV=6.0752 TT=656.43E-9 mfg=Philips type=silicon )
.MODEL PH_BZA856A D ( IS=323.83E-18 N=.97963 RS=.24251 IKF=6.4502 CJO=156.61E-12 M=.28517 VJ=.98457 ISR=9.2948E-9 NR=2.4186 BV=5.7918 IBV=.18506 TT=116.14E-9 mfg=Philips type=silicon )
.MODEL PH_BZA856AVL D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZA862A D ( IS=323.81E-18 N=.97963 RS=.24264 IKF=6.9002 CJO=140.64E-12 M=.29103 VJ=.92059 ISR=41.933E-9 NR=2.4186 BV=6.3692 IBV=.86917 TT=123.35E-9 mfg=Philips type=silicon )
.MODEL PH_BZA862AVL D ( IS = 3.644E-17 N = 0.9717 BV = 6.2 IBV = 0.001 RS = 0.5003 CJO = 1.815E-11 VJ = 0.7121 M = 0.3251 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZA868A D ( IS=323.81E-18 N=.97963 RS=.24264 IKF=6.9002 CJO=125.11E-12 M=.34068 VJ=1.2066 ISR=894.24E-12 NR=2.4186 BV=7.0126 IBV=2.4043 TT=115.42E-9 mfg=Philips type=silicon )
.MODEL PH_BZA868AVL D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZA956A D ( IS=274.79E-18 N=.99151 RS=.33553 IKF=8.8795 CJO=107.97E-12 M=.32308 VJ=.68909 ISR=1.1924E-6 NR=4.9950 BV=5.7434 IBV=.25951 TT=865.62E-9 mfg=Philips type=silicon )
.MODEL PH_BZA956AVL D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZA962A D ( IS=322.57E-18 N=.9961 RS=.31568 IKF=7.9489 CJO=89.986E-12 M=.33327 VJ=.75415 ISR=55.253E-9 NR=3.2011 BV=6.4066 IBV=2.9783 TT=865.62E-9 mfg=Philips type=silicon )
.MODEL PH_BZA962AVL D ( IS = 3.644E-17 N = 0.9717 BV = 6.2 IBV = 0.001 RS = 0.5003 CJO = 1.815E-11 VJ = 0.7121 M = 0.3251 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZA968A D ( IS=329.56E-18 N=.99805 RS=.3112 IKF=6.1249 CJO=77.958E-12 M=.34229 VJ=.77441 ISR=8.8151E-9 NR=4.9950 BV=7.0369 IBV=9.6192 TT=865.62E-9 mfg=Philips type=silicon )
.MODEL PH_BZA968AVL D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZV85-C33 D ( IS=110.88E-18 N=.92657 RS=.85899 IKF=149.75 CJO=16.677E-12 M=.34957 VJ=.66723 ISR=100.00E-12 BV=33.134 IBV=.37878 TT=2.2362E-6 mfg=Philips type=silicon )
.MODEL PH_BZX384-B10 D ( IS = 1.13E-14 N = 1.103 BV = 10 IBV = 0.005 RS = 0.4798 CJO = 6.004E-11 VJ = 0.6305 M = 0.3302 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B11 D ( IS = 1.13E-14 N = 1.103 BV = 11 IBV = 0.005 RS = 0.4798 CJO = 5.404E-11 VJ = 0.5891 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B12 D ( IS = 1.13E-14 N = 1.103 BV = 12 IBV = 0.005 RS = 0.4798 CJO = 4.928E-11 VJ = 0.575 M = 0.3292 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B13 D ( IS = 1.13E-14 N = 1.103 BV = 13 IBV = 0.005 RS = 0.4798 CJO = 4.377E-11 VJ = 0.5656 M = 0.3289 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B15 D ( IS = 1.13E-14 N = 1.103 BV = 15 IBV = 0.005 RS = 0.4798 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B16 D ( IS = 1.13E-14 N = 1.103 BV = 16 IBV = 0.005 RS = 0.4798 CJO = 3.509E-11 VJ = 0.6502 M = 0.3378 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B18 D ( IS = 1.13E-14 N = 1.103 BV = 18 IBV = 0.005 RS = 0.4798 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B20 D ( IS = 1.13E-14 N = 1.103 BV = 20 IBV = 0.005 RS = 0.4798 CJO = 2.915E-11 VJ = 0.635 M = 0.3362 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B22 D ( IS = 1.13E-14 N = 1.103 BV = 22 IBV = 0.005 RS = 0.4798 CJO = 2.701E-11 VJ = 0.7087 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B24 D ( IS = 1.13E-14 N = 1.103 BV = 24 IBV = 0.002 RS = 0.4798 CJO = 2.48E-11 VJ = 0.7142 M = 0.3513 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B27 D ( IS = 1.13E-14 N = 1.103 BV = 27 IBV = 0.002 RS = 0.4798 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B2V4 D ( IS = 1.033E-15 N = 1.001 BV = 2.4 IBV = 0.005 RS = 0.387 CJO = 3.615E-10 VJ = 0.5762 M = 0.2715 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B2V7 D ( IS = 1.033E-15 N = 1.001 BV = 2.7 IBV = 0.005 RS = 0.387 CJO = 3.518E-10 VJ = 0.6816 M = 0.3174 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B30 D ( IS = 1.13E-14 N = 1.103 BV = 30 IBV = 0.002 RS = 0.4798 CJO = 2.17E-011 VJ = 0.6718 M = 0.3465 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B33 D ( IS = 1.13E-14 N = 1.103 BV = 33 IBV = 0.002 RS = 0.4798 CJO = 2.019E-11 VJ = 0.7645 M = 0.3782 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B36 D ( IS = 1.13E-14 N = 1.103 BV = 36 IBV = 0.002 RS = 0.4798 CJO = 1.866E-11 VJ = 0.7591 M = 0.3771 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B39 D ( IS = 1.13E-14 N = 1.103 BV = 39 IBV = 0.002 RS = 0.4798 CJO = 1.772E-11 VJ = 0.7471 M = 0.3751 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B3V0 D ( IS = 1.033E-15 N = 1.001 BV = 3 IBV = 0.005 RS = 0.387 CJO = 3.346E-10 VJ = 0.6722 M = 0.3162 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B3V3 D ( IS = 1.033E-15 N = 1.001 BV = 3.3 IBV = 0.005 RS = 0.387 CJO = 3.162E-10 VJ = 0.6687 M = 0.3164 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B3V6 D ( IS = 1.033E-15 N = 1.001 BV = 3.6 IBV = 0.005 RS = 0.387 CJO = 3.062E-10 VJ = 0.6643 M = 0.3168 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B3V9 D ( IS = 1.033E-15 N = 1.001 BV = 3.9 IBV = 0.005 RS = 0.387 CJO = 2.82E-10 VJ = 0.6743 M = 0.3219 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B43 D ( IS = 1.13E-14 N = 1.103 BV = 43 IBV = 0.002 RS = 0.4798 CJO = 1.638E-11 VJ = 0.7517 M = 0.3762 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B47 D ( IS = 1.13E-14 N = 1.103 BV = 47 IBV = 0.002 RS = 0.4798 CJO = 1.707E-11 VJ = 0.888 M = 0.4248 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B4V3 D ( IS = 1.033E-15 N = 1.001 BV = 4.3 IBV = 0.005 RS = 0.387 CJO = 2.715E-10 VJ = 0.7721 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B4V7 D ( IS = 1.033E-15 N = 1.001 BV = 4.7 IBV = 0.005 RS = 0.387 CJO = 2.589E-10 VJ = 0.8029 M = 0.3636 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B51 D ( IS = 1.13E-14 N = 1.103 BV = 51 IBV = 0.002 RS = 0.4798 CJO = 1.602E-11 VJ = 0.8454 M = 0.4154 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B56 D ( IS = 1.13E-14 N = 1.103 BV = 56 IBV = 0.002 RS = 0.4798 CJO = 1.508E-11 VJ = 0.8856 M = 0.4177 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B5V1 D ( IS = 1.033E-15 N = 1.001 BV = 5.1 IBV = 0.005 RS = 0.387 CJO = 2.402E-10 VJ = 0.7934 M = 0.3578 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B5V6 D ( IS = 1.033E-15 N = 1.001 BV = 5.6 IBV = 0.005 RS = 0.387 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B62 D ( IS = 1.13E-14 N = 1.103 BV = 62 IBV = 0.002 RS = 0.4798 CJO = 1.403E-11 VJ = 0.8053 M = 0.4033 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B68 D ( IS = 1.13E-14 N = 1.103 BV = 68 IBV = 0.002 RS = 0.4798 CJO = 1.321E-11 VJ = 0.7877 M = 0.4021 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B6V2 D ( IS = 1.033E-15 N = 1.001 BV = 6.2 IBV = 0.005 RS = 0.387 CJO = 1.732E-10 VJ = 0.9334 M = 0.4321 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B6V8 D ( IS = 1.033E-15 N = 1.001 BV = 6.8 IBV = 0.005 RS = 0.387 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B75 D ( IS = 1.13E-14 N = 1.103 BV = 75 IBV = 0.002 RS = 0.4798 CJO = 1.246E-11 VJ = 0.822 M = 0.4052 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B7V5 D ( IS = 1.13E-14 N = 1.103 BV = 7.5 IBV = 0.005 RS = 0.4798 CJO = 8.767E-11 VJ = 0.5829 M = 0.3299 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B8V2 D ( IS = 1.13E-14 N = 1.103 BV = 8.2 IBV = 0.005 RS = 0.4798 CJO = 7.562E-11 VJ = 0.5765 M = 0.3298 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX384-B9V1 D ( IS = 1.13E-14 N = 1.103 BV = 9.1 IBV = 0.005 RS = 0.4798 CJO = 7.316E-11 VJ = 0.5667 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B10 D ( IS = 1.13E-14 N = 1.103 BV = 10 IBV = 0.005 RS = 0.4798 CJO = 6.004E-11 VJ = 0.6305 M = 0.3302 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B11 D ( IS = 1.13E-14 N = 1.103 BV = 11 IBV = 0.005 RS = 0.4798 CJO = 5.404E-11 VJ = 0.5891 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B12 D ( IS = 1.13E-14 N = 1.103 BV = 12 IBV = 0.005 RS = 0.4798 CJO = 4.928E-11 VJ = 0.575 M = 0.3292 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B13 D ( IS = 1.13E-14 N = 1.103 BV = 13 IBV = 0.005 RS = 0.4798 CJO = 4.377E-11 VJ = 0.5656 M = 0.3289 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B15 D ( IS = 1.13E-14 N = 1.103 BV = 15 IBV = 0.005 RS = 0.4798 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B16 D ( IS = 1.13E-14 N = 1.103 BV = 16 IBV = 0.005 RS = 0.4798 CJO = 3.509E-11 VJ = 0.6502 M = 0.3378 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B18 D ( IS = 1.13E-14 N = 1.103 BV = 18 IBV = 0.005 RS = 0.4798 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B20 D ( IS = 1.13E-14 N = 1.103 BV = 20 IBV = 0.005 RS = 0.4798 CJO = 2.915E-11 VJ = 0.635 M = 0.3362 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B22 D ( IS = 1.13E-14 N = 1.103 BV = 22 IBV = 0.005 RS = 0.4798 CJO = 2.701E-11 VJ = 0.7087 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B24 D ( IS = 1.13E-14 N = 1.103 BV = 24 IBV = 0.002 RS = 0.4798 CJO = 2.48E-11 VJ = 0.7142 M = 0.3513 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B27 D ( IS = 1.13E-14 N = 1.103 BV = 27 IBV = 0.002 RS = 0.4798 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B2V4 D ( IS = 1.033E-15 N = 1.001 BV = 2.4 IBV = 0.005 RS = 0.387 CJO = 3.615E-10 VJ = 0.5762 M = 0.2715 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B2V7 D ( IS = 1.033E-15 N = 1.001 BV = 2.7 IBV = 0.005 RS = 0.387 CJO = 3.518E-10 VJ = 0.6816 M = 0.3174 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B30 D ( IS = 1.13E-14 N = 1.103 BV = 30 IBV = 0.002 RS = 0.4798 CJO = 2.17E-011 VJ = 0.6718 M = 0.3465 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B33 D ( IS = 1.13E-14 N = 1.103 BV = 33 IBV = 0.002 RS = 0.4798 CJO = 2.019E-11 VJ = 0.7645 M = 0.3782 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B36 D ( IS = 1.13E-14 N = 1.103 BV = 36 IBV = 0.002 RS = 0.4798 CJO = 1.866E-11 VJ = 0.7591 M = 0.3771 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B39 D ( IS = 1.13E-14 N = 1.103 BV = 39 IBV = 0.002 RS = 0.4798 CJO = 1.772E-11 VJ = 0.7471 M = 0.3751 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B3V0 D ( IS = 1.033E-15 N = 1.001 BV = 3 IBV = 0.005 RS = 0.387 CJO = 3.346E-10 VJ = 0.6722 M = 0.3162 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B3V3 D ( IS = 1.033E-15 N = 1.001 BV = 3.3 IBV = 0.005 RS = 0.387 CJO = 3.162E-10 VJ = 0.6687 M = 0.3164 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B3V6 D ( IS = 1.033E-15 N = 1.001 BV = 3.6 IBV = 0.005 RS = 0.387 CJO = 3.062E-10 VJ = 0.6643 M = 0.3168 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B3V9 D ( IS = 1.033E-15 N = 1.001 BV = 3.9 IBV = 0.005 RS = 0.387 CJO = 2.82E-10 VJ = 0.6743 M = 0.3219 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B43 D ( IS = 1.13E-14 N = 1.103 BV = 43 IBV = 0.002 RS = 0.4798 CJO = 1.638E-11 VJ = 0.7517 M = 0.3762 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B47 D ( IS = 1.13E-14 N = 1.103 BV = 47 IBV = 0.002 RS = 0.4798 CJO = 1.707E-11 VJ = 0.888 M = 0.4248 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B4V3 D ( IS = 1.033E-15 N = 1.001 BV = 4.3 IBV = 0.005 RS = 0.387 CJO = 2.715E-10 VJ = 0.7721 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B4V7 D ( IS = 1.033E-15 N = 1.001 BV = 4.7 IBV = 0.005 RS = 0.387 CJO = 2.589E-10 VJ = 0.8029 M = 0.3636 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B51 D ( IS = 1.13E-14 N = 1.103 BV = 51 IBV = 0.002 RS = 0.4798 CJO = 1.602E-11 VJ = 0.8454 M = 0.4154 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B56 D ( IS = 1.13E-14 N = 1.103 BV = 56 IBV = 0.002 RS = 0.4798 CJO = 1.508E-11 VJ = 0.8856 M = 0.4177 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B5V1 D ( IS = 1.033E-15 N = 1.001 BV = 5.1 IBV = 0.005 RS = 0.387 CJO = 2.402E-10 VJ = 0.7934 M = 0.3578 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B5V6 D ( IS = 1.033E-15 N = 1.001 BV = 5.6 IBV = 0.005 RS = 0.387 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B62 D ( IS = 1.13E-14 N = 1.103 BV = 62 IBV = 0.002 RS = 0.4798 CJO = 1.403E-11 VJ = 0.8053 M = 0.4033 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B68 D ( IS = 1.13E-14 N = 1.103 BV = 68 IBV = 0.002 RS = 0.4798 CJO = 1.321E-11 VJ = 0.7877 M = 0.4021 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B6V2 D ( IS = 1.033E-15 N = 1.001 BV = 6.2 IBV = 0.005 RS = 0.387 CJO = 1.732E-10 VJ = 0.9334 M = 0.4321 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B6V8 D ( IS = 1.033E-15 N = 1.001 BV = 6.8 IBV = 0.005 RS = 0.387 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B75 D ( IS = 1.13E-14 N = 1.103 BV = 75 IBV = 0.002 RS = 0.4798 CJO = 1.246E-11 VJ = 0.822 M = 0.4052 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B7V5 D ( IS = 1.13E-14 N = 1.103 BV = 7.5 IBV = 0.005 RS = 0.4798 CJO = 8.767E-11 VJ = 0.5829 M = 0.3299 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B8V2 D ( IS = 1.13E-14 N = 1.103 BV = 8.2 IBV = 0.005 RS = 0.4798 CJO = 7.562E-11 VJ = 0.5765 M = 0.3298 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX585-B9V1 D ( IS = 1.13E-14 N = 1.103 BV = 9.1 IBV = 0.005 RS = 0.4798 CJO = 7.316E-11 VJ = 0.5667 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX84C3V3 D ( IS = 7.035E-16 N = 0.9809 BV = 3.3 IBV = 0.005 RS = 0.3487 CJO = 3.162E-10 VJ = 0.6687 M = 0.3164 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX84C4V3 D ( IS = 7.035E-16 N = 0.9809 BV = 4.3 IBV = 0.005 RS = 0.3487 CJO = 2.715E-10 VJ = 0.7721 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX84C75 D ( IS = 9.794E-15 N = 1.101 BV = 75 IBV = 0.002 RS = 0.3363 CJO = 1.246E-11 VJ = 0.822 M = 0.4052 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B10 D ( IS = 5.229E-15 N = 1.061 BV = 10 IBV = 0.005 RS = 0.4467 CJO = 6.004E-11 VJ = 0.6305 M = 0.3302 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B11 D ( IS = 5.229E-15 N = 1.061 BV = 11 IBV = 0.005 RS = 0.4467 CJO = 5.404E-11 VJ = 0.5891 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B12 D ( IS = 5.229E-15 N = 1.061 BV = 12 IBV = 0.005 RS = 0.4467 CJO = 4.928E-11 VJ = 0.575 M = 0.3292 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B13 D ( IS = 5.229E-15 N = 1.061 BV = 13 IBV = 0.005 RS = 0.4467 CJO = 4.377E-11 VJ = 0.5656 M = 0.3289 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B15 D ( IS = 5.229E-15 N = 1.061 BV = 15 IBV = 0.005 RS = 0.4467 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B16 D ( IS = 5.229E-15 N = 1.061 BV = 16 IBV = 0.005 RS = 0.4467 CJO = 3.509E-11 VJ = 0.6502 M = 0.3378 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B18 D ( IS = 5.229E-15 N = 1.061 BV = 18 IBV = 0.005 RS = 0.4467 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B20 D ( IS = 5.229E-15 N = 1.061 BV = 20 IBV = 0.005 RS = 0.4467 CJO = 2.915E-11 VJ = 0.635 M = 0.3362 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B22 D ( IS = 5.229E-15 N = 1.061 BV = 22 IBV = 0.005 RS = 0.4467 CJO = 2.701E-11 VJ = 0.7087 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B24 D ( IS = 5.229E-15 N = 1.061 BV = 24 IBV = 0.002 RS = 0.4467 CJO = 2.48E-11 VJ = 0.7142 M = 0.3513 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B27 D ( IS = 5.229E-15 N = 1.061 BV = 27 IBV = 0.002 RS = 0.4467 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B2V4 D ( IS = 7.066E-16 N = 0.9643 BV = 2.4 IBV = 0.005 RS = 0.2544 CJO = 3.615E-10 VJ = 0.5762 M = 0.2715 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B2V7 D ( IS = 7.066E-16 N = 0.9643 BV = 2.7 IBV = 0.005 RS = 0.2544 CJO = 3.518E-10 VJ = 0.6816 M = 0.3174 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B30 D ( IS = 5.229E-15 N = 1.061 BV = 30 IBV = 0.002 RS = 0.4467 CJO = 2.17E-011 VJ = 0.6718 M = 0.3465 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B33 D ( IS = 5.229E-15 N = 1.061 BV = 33 IBV = 0.002 RS = 0.4467 CJO = 2.019E-11 VJ = 0.7645 M = 0.3782 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B36 D ( IS = 5.229E-15 N = 1.061 BV = 36 IBV = 0.002 RS = 0.4467 CJO = 1.866E-11 VJ = 0.7591 M = 0.3771 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B39 D ( IS = 5.229E-15 N = 1.061 BV = 39 IBV = 0.002 RS = 0.4467 CJO = 1.772E-11 VJ = 0.7471 M = 0.3751 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B3V0 D ( IS = 7.066E-16 N = 0.9643 BV = 3 IBV = 0.005 RS = 0.2544 CJO = 3.346E-10 VJ = 0.6722 M = 0.3162 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B3V3 D ( IS = 7.066E-16 N = 0.9643 BV = 3.3 IBV = 0.005 RS = 0.2544 CJO = 3.162E-10 VJ = 0.6687 M = 0.3164 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B3V6 D ( IS = 7.066E-16 N = 0.9643 BV = 3.6 IBV = 0.005 RS = 0.2544 CJO = 3.062E-10 VJ = 0.6643 M = 0.3168 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B3V9 D ( IS = 7.066E-16 N = 0.9643 BV = 3.9 IBV = 0.005 RS = 0.2544 CJO = 2.82E-10 VJ = 0.6743 M = 0.3219 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B43 D ( IS = 5.229E-15 N = 1.061 BV = 43 IBV = 0.002 RS = 0.4467 CJO = 1.638E-11 VJ = 0.7517 M = 0.3762 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B47 D ( IS = 5.229E-15 N = 1.061 BV = 47 IBV = 0.002 RS = 0.4467 CJO = 1.707E-11 VJ = 0.888 M = 0.4248 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B4V3 D ( IS = 7.066E-16 N = 0.9643 BV = 4.3 IBV = 0.005 RS = 0.2544 CJO = 2.715E-10 VJ = 0.7721 M = 0.3557 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B4V7 D ( IS = 7.066E-16 N = 0.9643 BV = 4.7 IBV = 0.005 RS = 0.2544 CJO = 2.589E-10 VJ = 0.8029 M = 0.3636 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B51 D ( IS = 5.229E-15 N = 1.061 BV = 51 IBV = 0.002 RS = 0.4467 CJO = 1.602E-11 VJ = 0.8454 M = 0.4154 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B56 D ( IS = 5.229E-15 N = 1.061 BV = 56 IBV = 0.002 RS = 0.4467 CJO = 1.508E-11 VJ = 0.8856 M = 0.4177 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B5V1 D ( IS = 7.066E-16 N = 0.9643 BV = 5.1 IBV = 0.005 RS = 0.2544 CJO = 2.402E-10 VJ = 0.7934 M = 0.3578 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B5V6 D ( IS = 7.066E-16 N = 0.9643 BV = 5.6 IBV = 0.005 RS = 0.2544 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B62 D ( IS = 5.229E-15 N = 1.061 BV = 62 IBV = 0.002 RS = 0.4467 CJO = 1.403E-11 VJ = 0.8053 M = 0.4033 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B68 D ( IS = 5.229E-15 N = 1.061 BV = 68 IBV = 0.002 RS = 0.4467 CJO = 1.321E-11 VJ = 0.7877 M = 0.4021 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B6V2 D ( IS = 7.066E-16 N = 0.9643 BV = 6.2 IBV = 0.005 RS = 0.2544 CJO = 1.732E-10 VJ = 0.9334 M = 0.4321 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B6V8 D ( IS = 7.066E-16 N = 0.9643 BV = 6.8 IBV = 0.005 RS = 0.2544 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B75 D ( IS = 5.229E-15 N = 1.061 BV = 75 IBV = 0.002 RS = 0.4467 CJO = 1.246E-11 VJ = 0.822 M = 0.4052 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B7V5 D ( IS = 5.229E-15 N = 1.061 BV = 7.5 IBV = 0.005 RS = 0.4467 CJO = 8.767E-11 VJ = 0.5829 M = 0.3299 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B8V2 D ( IS = 5.229E-15 N = 1.061 BV = 8.2 IBV = 0.005 RS = 0.4467 CJO = 7.562E-11 VJ = 0.5765 M = 0.3298 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_BZX884-B9V1 D ( IS = 5.229E-15 N = 1.061 BV = 9.1 IBV = 0.005 RS = 0.4467 CJO = 7.316E-11 VJ = 0.5667 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PDZ10B D ( IS = 9.794E-15 N = 1.101 BV = 10 IBV = 0.005 RS = 0.3363 CJO = 6.004E-11 VJ = 0.6305 M = 0.3302 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PDZ11B D ( IS = 9.794E-15 N = 1.101 BV = 11 IBV = 0.005 RS = 0.3363 CJO = 5.404E-11 VJ = 0.5891 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PDZ4.7B D ( IS = 1.033E-15 N = 1.001 BV = 4.7 IBV = 0.005 RS = 0.387 CJO = 2.589E-10 VJ = 0.8029 M = 0.3636 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PDZ5.6B D ( IS = 1.777E-15 N = 1.015 BV = 5.6 IBV = 0.00025 RS = 0.3502 CJO = 1.298E-10 VJ = 0.6612 M = 0.3228 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PDZ9.1B D ( IS = 9.794E-15 N = 1.101 BV = 9.1 IBV = 0.005 RS = 0.3363 CJO = 7.316E-11 VJ = 0.5667 M = 0.3295 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VL1BA D ( IS = 9.794E-15 N = 1.101 BV = 15 IBV = 0.005 RS = 0.3363 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VL2BT D ( IS = 9.794E-15 N = 1.101 BV = 15 IBV = 0.005 RS = 0.3363 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VS1UB D ( IS = 1.13E-14 N = 1.103 BV = 15 IBV = 0.005 RS = 0.4798 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VS2UAT D ( IS = 9.794E-15 N = 1.101 BV = 15 IBV = 0.005 RS = 0.3363 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VS2UQ D ( IS = 9.72E-15 N = 1.088 BV = 15.4 IBV = 0.005 RS = 0.2663 CJO = 4.023E-11 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD12VS2UT D ( IS = 9.794E-015 N = 1.101 BV = 15 IBV = 0.005 RS = 0.3363 CJO = 4.023E-011 VJ = 0.6144 M = 0.3297 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VL1BA D ( IS = 9.794E-15 N = 1.101 BV = 18 IBV = 0.005 RS = 0.3363 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VL2BT D ( IS = 9.794E-15 N = 1.101 BV = 18 IBV = 0.005 RS = 0.3363 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VS1UB D ( IS = 1.13E-14 N = 1.103 BV = 18 IBV = 0.005 RS = 0.4798 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VS2UAT D ( IS = 9.794E-15 N = 1.101 BV = 18 IBV = 0.005 RS = 0.3363 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VS2UQ D ( IS = 9.794E-15 N = 1.101 BV = 18 IBV = 0.005 RS = 0.3363 CJO = 3.17E-11 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD15VS2UT D ( IS = 9.794E-015 N = 1.101 BV = 18 IBV = 0.005 RS = 0.3363 CJO = 3.17E-011 VJ = 0.6421 M = 0.3327 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD1CAN D ( IS = 9.794E-15 N = 1.101 BV = 27 IBV = 0.002 RS = 0.3363 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VL1BA D ( IS = 9.794E-15 N = 1.101 BV = 27 IBV = 0.002 RS = 0.3363 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VL2BT D ( IS = 9.794E-15 N = 1.101 BV = 27 IBV = 0.002 RS = 0.3363 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VS1UB D ( IS = 1.13E-14 N = 1.103 BV = 27 IBV = 0.002 RS = 0.4798 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VS2UAT D ( IS = 9.794E-15 N = 1.101 BV = 27 IBV = 0.002 RS = 0.3363 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VS2UQ D ( IS = 9.794E-15 N = 1.101 BV = 27 IBV = 0.002 RS = 0.3363 CJO = 2.233E-11 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD24VS2UT D ( IS = 9.794E-015 N = 1.101 BV = 27 IBV = 0.005 RS = 0.3363 CJO = 2.233E-011 VJ = 0.7107 M = 0.3546 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L1BA D ( IS = 7.035E-16 N = 0.9809 BV = 5.6 IBV = 0.005 RS = 0.3487 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L2BT D ( IS = 7.035E-16 N = 0.9809 BV = 5.6 IBV = 0.005 RS = 0.3487 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L2UM D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L4UG D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L4UW D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L5UV D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3L5UY D ( IS = 3.644E-17 N = 0.9717 BV = 5.6 IBV = 0.001 RS = 0.5003 CJO = 2.136E-11 VJ = 0.7025 M = 0.3242 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3S1UB D ( IS = 1.033E-15 N = 1.001 BV = 5.6 IBV = 0.005 RS = 0.387 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3S2UAT D ( IS = 7.035E-16 N = 0.9809 BV = 5.6 IBV = 0.005 RS = 0.3487 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3S2UQ D ( IS = 3.134E-16 N = 0.9403 BV = 5.6 IBV = 0.005 RS = 0.2549 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3S2UT D ( IS = 7.035E-16 N = 0.9809 BV = 5.6 IBV = 0.005 RS = 0.3487 CJO = 1.961E-10 VJ = 0.9187 M = 0.423 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD3V3V4UG D ( IS = 2.497E-17 N = 1.003 BV = 5.6 IBV = 0.001 RS = 0.5053 CJO = 1.561E-11 VJ = 0.6327 M = 0.2904 mfg=Philips type=zener )
.MODEL PH_PESD3V3V4UW D ( IS = 2.497E-17 N = 1.003 BV = 5.6 IBV = 0.001 RS = 0.5053 CJO = 1.561E-11 VJ = 0.6327 M = 0.2904 mfg=Philips type=zener )
.MODEL PH_PESD5V0L1BA D ( IS = 7.035E-16 N = 0.9809 BV = 6.8 IBV = 0.005 RS = 0.3487 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L2BT D ( IS = 7.035E-16 N = 0.9809 BV = 6.8 IBV = 0.005 RS = 0.3487 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L2UM D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L4UG D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L4UW D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L5UV D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L5UY D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L6UAS D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L6US D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L7BAS D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0L7BS D ( IS = 3.644E-17 N = 0.9717 BV = 6.8 IBV = 0.001 RS = 0.5003 CJO = 1.641E-11 VJ = 0.8979 M = 0.33 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0S1UB D ( IS = 1.033E-15 N = 1.001 BV = 6.8 IBV = 0.005 RS = 0.387 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0S2UAT D ( IS = 7.035E-16 N = 0.9809 BV = 6.8 IBV = 0.005 RS = 0.3487 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0S2UQ D ( IS = 3.02E-16 N = 0.9388 BV = 5.6 IBV = 0.005 RS = 0.2559 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V0V4UG D ( IS = 3.997E-17 N = 1.012 BV = 6.8 IBV = 0.001 RS = 1.445 CJO = 1.217E-11 VJ = 0.6509 M = 0.2841 mfg=Philips type=zener )
.MODEL PH_PESD5V2S18U D ( IS = 2.779E-16 N = 0.9976 BV = 6.7 IBV = 0.001 RS = 0.2888 CJO = 1.025E-10 VJ = 0.7664 M = 0.3438 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5V2S2UT D ( IS = 7.035E-16 N = 0.9809 BV = 6.8 IBV = 0.005 RS = 0.3487 CJO = 1.519E-10 VJ = 0.9041 M = 0.4027 FC = 0.5 mfg=Philips type=zener )
.MODEL PH_PESD5VOV4UW D ( IS = 3.997E-17 N = 1.012 BV = 6.8 IBV = 0.001 RS = 1.445 CJO = 1.217E-11 VJ = 0.6509 M = 0.2841 mfg=Philips type=zener )
.MODEL PH_PLVA2656A D ( IS=1.2302E-15 N=.99169 RS=.4793 IKF=49.525E-3 CJO=125.26E-12 M=.33643 VJ=.68657 ISR=32.826E-9 BV=5.7651 IBV=3.2718 TT=104.45E-9 mfg=Philips type=silicon )
.MODEL PH_PLVA650A D ( IS=535.74E-18 N=1.0029 RS=.29276 IKF=2.5050 CJO=119.42E-12 M=.32565 VJ=.62169 ISR=216.91E-9 NR=4.9950 BV=5.1893 IBV=.21213 TT=132.15E-9 mfg=Philips type=silicon )
.MODEL PH_PMBD6050 D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=1.6725E-9 NR=4.9950 BV=139.42 IBV=34.486E-3 TT=4.5000E-9 mfg=Philips type=silicon )
.MODEL PH_PMBD7000 D ( IS=6.0289E-9 N=2.1283 RS=1.0000E-3 IKF=37.638E-3 CJO=593.63E-15 M=.1 VJ=.68774 ISR=2.0646E-9 NR=4.9950 BV=113.60 IBV=10 TT=5.7708E-9 mfg=Philips type=silicon )
.MODEL PH_PMBD7100 D ( IS = 3.622E-9 N = 1.865 BV = 110 IBV = 1E-5 RS = 0.9623 CJO = 5.936E-13 VJ = 0.6877 M = 0.1 FC = 0.5 TT = 3.246E-9 mfg=Philips type=silicon )
.MODEL PH_1PS10SB62 D ( IS = 4E-10 N = 0.9529 BV = 43 IBV = 1E-6 RS = 131.3 CJO = 3.732E-13 VJ = 0.117 M = 0.9339 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS10SB63 D ( IS = 2.655E-7 N = 1.033 BV = 6 IBV = 5E-5 RS = 20.51 CJO = 3.376E-13 VJ = 0.02199 M = 0.0446 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS10SB82 D ( IS = 1.042E-8 N = 1.029 BV = 17 IBV = 0.001 RS = 5.567 CJO = 9.779E-13 VJ = 0.2925 M = 0.194 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS66SB17 D ( IS = 1.419E-09 N = 1.022 BV = 6 IBV = 2.45E-06 RS = 5.112 CJO = 7.662E-13 VJ = 0.1681 M = 0.1995 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS66SB62 D ( IS = 4E-10 N = 0.9529 BV = 43 IBV = 0.0001 RS = 131.3 CJO = 3.834E-13 VJ = 0.08942 M = 0.08687 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS66SB63 D ( IS = 2.655E-07 N = 1.033 BV = 6 IBV = 5E-05 RS = 20.51 CJO = 3.52E-13 VJ = 0.007297 M = 0.05795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS66SB82 D ( IS = 1.042E-8 N = 1.029 BV = 17 IBV = 0.001 RS = 5.567 CJO = 9.779E-13 VJ = 0.2925 M = 0.194 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS70SB10 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB14 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB15 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB16 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB20 D( IS = 4.291E-06 N = 1.002 BV = 44 IBV = 3.0E-05 RS = 0.3772 CJO = 7.8E-11 VJ = 0.4015 M = 0.508 FC = 0.1 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB40 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB44 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB45 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB46 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS70SB82 D ( IS = 1.042E-08 N = 1.029 BV = 20 IBV = 0.001 RS = 5.567 CJO = 1.029E-12 VJ = 0.2159 M = 0.1731 FC = 0 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS70SB84 D ( IS = 1.042E-08 N = 1.029 BV = 20 IBV = 0.001 RS = 5.567 CJO = 1.029E-12 VJ = 0.2159 M = 0.1731 FC = 0 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS70SB85 D ( IS = 1.042E-08 N = 1.029 BV = 20 IBV = 0.001 RS = 5.567 CJO = 1.029E-12 VJ = 0.2159 M = 0.1731 FC = 0 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS70SB86 D ( IS = 1.042E-08 N = 1.029 BV = 20 IBV = 0.001 RS = 5.567 CJO = 1.029E-12 VJ = 0.2159 M = 0.1731 FC = 0 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS74SB23 D ( IS = 6.984E-06 N = 1.023 BV = 30 IBV = 0.0002402 RS = 0.1574 CJO = 3.075E-10 VJ = 0.6615 M = 0.6098 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS74SB43 D ( IS = 4.9E-06 N = 1.001 BV = 40 IBV = 6E-05 RS = 0.108 CJO = 3.791E-10 VJ = 0.103 M = 0.4704 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS75SB45 D( IS = 9.114E-09 N = 1.006 BV = 45 IBV = 7.8E-05 RS = 4.563 CJO = 3.895E-12 VJ = 0.3192 M = 0.4008 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS76SB10 D( IS = 2.548E-07 N = 1.02 BV = 33 IBV = 1.251E-06 RS = 2.582 CJO = 9.92E-12 VJ = 0.317 M = 0.4411 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS76SB17 D( IS = 1.419E-09 N = 1.022 BV = 6 IBV = 2.45E-06 RS = 5.112 CJO = 7.867E-13 VJ = 0.1043 M = 0.1439 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS76SB21 D ( ( IS = 1.009E-06 N = 1.017 BV = 44 IBV = 0.001611 RS = 0.6578 CJO = 3.76E-11 VJ = 0.274 M = 0.4381 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_1PS76SB40 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS76SB62 D ( IS = 4E-10 N = 0.9529 BV = 43 IBV = 0.0001 RS = 131.3 CJO = 4.181E-13 VJ = 0.1122 M = 0.08766 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS76SB70 D( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS79SB10 D( IS = 2.36E-07 N = 1.009 BV = 33 IBV = 0.001 RS = 2.633 CJO = 9.53E-12 VJ = 0.2034 M = 0.3811 FC = 0.6435 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_1PS79SB17 D ( IS = 1.419E-9 N = 1.022 BV = 6 IBV = 2.45E-6 RS = 5.112 CJO = 7.662E-13 VJ = 0.1681 M = 0.1995 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS79SB30 D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS79SB31 D ( IS = 9.539E-07 N = 1.007 BV = 35 IBV = 4E-05 RS = 0.4678 CJO = 3.518E-11 VJ = 0.3193 M = 0.4687 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS79SB40 D ( IS = 8.361E-09 N = 1.003 BV = 44 IBV = 8E-07 RS = 5.031 CJO = 3.8E-12 VJ = 0.1119 M = 0.2915 FC = 1 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS79SB62 D ( IS = 4E-10 N = 0.9529 BV = 43 IBV = 0.0001 RS = 131.3 CJO = 4.077E-13 VJ = 0.1032 M = 0.09482 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS79SB63 D ( IS = 2.655E-07 N = 1.033 BV = 6 IBV = 5E-05 RS = 20.51 CJO = 3.52E-13 VJ = 0.007297 M = 0.05795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS88SB48 D ( IS = 9.649E-09 N = 1.013 BV = 1000 IBV = 0.001 RS = 4.999 CJO = 3.928E-12 VJ = 0.2057 M = 0.3426 FC = 4.441E-16 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS88SB82 D ( IS = 1.042E-08 N = 1.029 BV = 20 IBV = 0.001 RS = 5.567 CJO = 1.029E-12 VJ = 0.2159 M = 0.1731 FC = 0 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_1PS89SB74 D ( IS = 2.775E-09 N = 1.021 BV = 77 IBV = 1.67E-07 RS = 27.73 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS240 D ( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 3.89E-12 VJ = 0.1217 M = 0.2899 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS40-04 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-04W D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-05 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-05V D( IS = 9.114E-09 N = 1.006 BV = 45 IBV = 7.8E-05 RS = 4.563 CJO = 3.895E-12 VJ = 0.3192 M = 0.4008 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-05W D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-06 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-06W D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40-07 D ( IS = 8.361E-09 N = 1.003 BV = 44 IBV = 8E-07 RS = 5.031 CJO = 3.8E-12 VJ = 0.1119 M = 0.2915 FC = 1 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS40-07V D ( IS = 8.361E-09 N = 1.003 BV = 44 IBV = 8E-07 RS = 5.031 CJO = 3.8E-12 VJ = 0.1119 M = 0.2915 FC = 1 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS40 D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS40H D ( IS = 8.361E-09 N = 1.003 BV = 44 IBV = 8E-07 RS = 5.031 CJO = 3.8E-12 VJ = 0.1119 M = 0.2915 FC = 1 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS40W D( IS = 1.419E-08 N = 1.025 BV = 44 IBV = 1.255E-07 RS = 4.942 CJO = 4.046E-12 VJ = 0.323 M = 0.4154 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS70-07V D ( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS70 D( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAS70H D ( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS70L D ( IS = 3.22E-9 N = 1.018 BV = 77 IBV = 1.67E-7 RS = 20.89 CJO = 1.608E-12 VJ = 0.3891 M = 0.3683 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS70VV D ( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAS70W D( IS = 3.22E-09 N = 1.018 BV = 77 IBV = 1.67E-07 RS = 20.89 CJO = 1.655E-12 VJ = 0.349 M = 0.3583 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT120A (D IS = 6.984E-06 N = 1.023 BV = 30 IBV = 0.0002402 RS = 0.1574 CJO = 3.075E-10 VJ = 0.6615 M = 0.6098 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_BAT120C (D IS = 6.984E-06 N = 1.023 BV = 30 IBV = 0.0002402 RS = 0.1574 CJO = 3.075E-10 VJ = 0.6615 M = 0.6098 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_BAT120S (D IS = 6.984E-06 N = 1.023 BV = 30 IBV = 0.0002402 RS = 0.1574 CJO = 3.075E-10 VJ = 0.6615 M = 0.6098 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_BAT160A D ( IS = 5E-7 N = 0.9751 BV = 66 IBV = 0.0004 RS = 0.3422 CJO = 1.75E-10 VJ = 0.3761 M = 0.4725 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT160C D ( IS = 5E-7 N = 0.9751 BV = 66 IBV = 0.0004 RS = 0.3422 CJO = 1.75E-10 VJ = 0.3761 M = 0.4725 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT160S D ( IS = 5E-7 N = 0.9751 BV = 66 IBV = 0.0004 RS = 0.3422 CJO = 1.75E-10 VJ = 0.3761 M = 0.4725 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT17 D ( IS = 1.419E-09 N = 1.022 BV = 6 IBV = 2.45E-06 RS = 5.112 CJO = 7.867E-13 VJ = 0.1043 M = 0.1439 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54A D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54AW D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 7E-9 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54C D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54CM D ( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54CV D ( IS = 2.117E-7 N = 1.016 BV = 36 IBV = 1.196E-6 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54CW D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 7E-9 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54H D ( IS = 2.36E-07 N = 1.009 BV = 33 IBV = 0.001 RS = 2.633 CJO = 9.53E-12 VJ = 0.2034 M = 0.3811 FC = 0.6435 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54L D ( IS = 2.117E-7 N = 1.016 BV = 36 IBV = 1.196E-6 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54S D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54SW D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 7E-9 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54VV D ( IS = 2.36E-07 N = 1.009 BV = 33 IBV = 0.001 RS = 2.633 CJO = 9.53E-12 VJ = 0.2034 M = 0.3811 FC = 0.6435 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT54W D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 7E-9 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT54XY D ( IS = 2.019E-007 N = 1.003 BV = 33 IBV = 1.5E-006 RS = 2.759 CJO = 7.258E-012 VJ = 0.2049 M = 0.3577 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT720 D ( IS = 1.281E-06 N = 1.009 BV = 44 IBV = 2.21E-05 RS = 0.3093 CJO = 8.133E-11 VJ = 0.4519 M = 0.5304 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT721 D( IS = 1.009E-06 N = 1.017 BV = 44 IBV = 0.001611 RS = 0.6578 CJO = 3.76E-11 VJ = 0.274 M = 0.4381 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT721A D( IS = 1.009E-06 N = 1.017 BV = 44 IBV = 0.001611 RS = 0.6578 CJO = 3.76E-11 VJ = 0.274 M = 0.4381 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT721C D( IS = 1.009E-06 N = 1.017 BV = 44 IBV = 0.001611 RS = 0.6578 CJO = 3.76E-11 VJ = 0.274 M = 0.4381 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT721S D( IS = 1.009E-06 N = 1.017 BV = 44 IBV = 0.001611 RS = 0.6578 CJO = 3.76E-11 VJ = 0.274 M = 0.4381 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT74 D( IS = 2.548E-07 N = 1.02 BV = 33 IBV = 1.251E-06 RS = 2.582 CJO = 9.92E-12 VJ = 0.317 M = 0.4411 FC = 0.5 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT74V D ( IS = 2.36E-07 N = 1.009 BV = 33 IBV = 0.001 RS = 2.633 CJO = 9.53E-12 VJ = 0.2034 M = 0.3811 FC = 0.6435 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT754L D ( IS = 2.993E-07 N = 1.01 BV = 30 IBV = 1.5E-06 RS = 2.734 CJO = 9.228E-12 VJ = 0.3033 M = 0.4131 FC = 0.5178 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT760 D ( ( IS = 1.686E-06 N = 1.015 BV = 21 IBV = 1E-06 RS = 0.1249 CJO = 9.086E-11 VJ = 0.1939 M = 0.4542 FC = 1 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_BAT85 D( IS = 2.117E-07 N = 1.016 BV = 36 IBV = 1.196E-06 RS = 2.637 CJO = 1.114E-11 VJ = 0.2013 M = 0.3868 FC = 0 TT = 0 EG = 0.69 XTI = 2) mfg=Philips type=schottky )
.MODEL PH_BAT854AW D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT854CW D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT854SW D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT854W D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_BAT960 D ( ( IS = 1.686E-06 N = 1.015 BV = 21 IBV = 1E-06 RS = 0.1249 CJO = 9.086E-11 VJ = 0.1939 M = 0.4542 FC = 1 TT = 0 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_PMBD354 D ( IS = 1.419E-09 N = 1.022 BV = 6 IBV = 2.45E-06 RS = 5.112 CJO = 7.867E-13 VJ = 0.1043 M = 0.1439 FC = 0.5 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1020EA D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1020EH D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1020EJ D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1020EV D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1030EH D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG1030EJ D ( IS = 0.000259 N = 1.014 RS = 0.0635 BV = 12 IBV = 0.01 CJO = 2.553E-10 VJ = 0.0331 M = 0.3788 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005AEA D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005AEL D ( IS = 8.724E-5 N = 0.9699 BV = 22 IBV = 0.0004 RS = 0.2728 CJO = 2.999E-11 VJ = 0.2604 M = 0.3755 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005AEV D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005EB D ( IS = 9.985E-7 N = 0.9283 BV = 32 IBV = 0.001 RS = 0.2146 CJO = 6.105E-11 VJ = 0.1 M = 0.4159 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005EH D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005EJ D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005EL D ( IS = 9.985E-7 N = 0.9283 BV = 32 IBV = 0.001 RS = 0.2146 CJO = 6.105E-11 VJ = 0.1 M = 0.4159 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2005ET D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010AEB D ( IS = 8.724E-5 N = 0.9699 BV = 22 IBV = 0.0004 RS = 0.2728 CJO = 2.999E-11 VJ = 0.2604 M = 0.3755 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010AEH D ( IS = 5.409E-6 N = 1.02 BV = 22 IBV = 5E-5 RS = 0.05676 CJO = 1.908E-10 VJ = 0.3408 M = 0.4863 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010AEJ D ( IS = 1.686E-06 N = 1.015 BV = 24 IBV = 0.001 RS = 0.1249 CJO = 6.969E-11 VJ = 0.4003 M = 0.4944 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010BEA D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010BEV D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010EA D ( ( IS = 1.686E-06 N = 1.015 BV = 21 IBV = 1E-06 RS = 0.1249 CJO = 9.086E-11 VJ = 0.1939 M = 0.4542 FC = 1 EG = 0.69 XTI = 2 ) mfg=Philips type=schottky )
.MODEL PH_PMEG2010EH D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2010EJ D ( IS = 3.334E-6 N = 0.9791 BV = 22 IBV = 0.0001 RS = 0.08222 CJO = 1.266E-10 VJ = 0.3619 M = 0.5 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2015EA D ( IS = 1.686E-06 N = 1.015 BV = 24 IBV = 0.001 RS = 0.1249 CJO = 6.969E-11 VJ = 0.4003 M = 0.4944 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2015EH D ( IS = 1.686E-06 N = 1.015 BV = 24 IBV = 0.001 RS = 0.1249 CJO = 6.969E-11 VJ = 0.4003 M = 0.4944 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2015EJ D ( IS = 1.686E-06 N = 1.015 BV = 24 IBV = 0.001 RS = 0.1249 CJO = 6.969E-11 VJ = 0.4003 M = 0.4944 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2015EV D ( IS = 1.175E-6 N = 0.9841 BV = 24 IBV = 0.001 RS = 0.1476 CJO = 7.035E-11 VJ = 0.3891 M = 0.4845 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2020AEA D ( IS = 5.409E-6 N = 1.02 BV = 22 IBV = 5E-5 RS = 0.05676 CJO = 1.908E-10 VJ = 0.3408 M = 0.4863 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG2020EJ D ( IS = 5.409E-6 N = 1.02 BV = 22 IBV = 5E-5 RS = 0.05676 CJO = 1.908E-10 VJ = 0.3408 M = 0.4863 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3002AEB D ( IS = 9.539E-07 N = 1.007 BV = 35 IBV = 4E-05 RS = 0.4678 CJO = 3.518E-11 VJ = 0.3193 M = 0.4687 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3002AEL D ( IS = 9.539E-07 N = 1.007 BV = 35 IBV = 4E-05 RS = 0.4678 CJO = 3.518E-11 VJ = 0.3193 M = 0.4687 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3002TV D ( IS = 9.539E-07 N = 1.007 BV = 35 IBV = 4E-05 RS = 0.4678 CJO = 3.518E-11 VJ = 0.3193 M = 0.4687 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3005AEA D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3005AEV D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3005EH D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3005EJ D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3005ET D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3010BEA D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3010BEV D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3010CEJ D ( IS = 3.735E-007 N = 0.994 BV = 33 IBV = 1E-005 RS = 0.07992 CJO = 1.645E-010 VJ = 0.4041 M = 0.4946 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3010EH D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3010EJ D ( IS = 2.936E-6 N = 0.9839 BV = 33 IBV = 7.5E-5 RS = 0.1166 CJO = 1.068E-10 VJ = 0.3459 M = 0.4948 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3015EH D ( IS = 1.05E-5 N = 0.998 BV = 33 IBV = 0.0004 RS = 0.08651 CJO = 1.189E-10 VJ = 0.3379 M = 0.4795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3015EJ D ( IS = 1.05E-5 N = 0.998 BV = 33 IBV = 0.0004 RS = 0.08651 CJO = 1.189E-10 VJ = 0.3379 M = 0.4795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3015EV D ( IS = 1.05E-5 N = 0.998 BV = 33 IBV = 0.0004 RS = 0.08651 CJO = 1.189E-10 VJ = 0.3379 M = 0.4795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3020EH D ( IS = 1.05E-5 N = 0.998 BV = 33 IBV = 0.0004 RS = 0.08651 CJO = 1.189E-10 VJ = 0.3379 M = 0.4795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG3020EJ D ( IS = 1.05E-5 N = 0.998 BV = 33 IBV = 0.0004 RS = 0.08651 CJO = 1.189E-10 VJ = 0.3379 M = 0.4795 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4002EL D ( IS = 8E-08 N = 1.012 BV = 45 IBV = 0.0001 RS = 0.8243 CJO = 2.515E-11 VJ = 0.4182 M = 0.4941 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4005AEA D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4005AEV D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4005EH D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4005EJ D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4005ET D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4010BEA D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4010BEV D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4010CEJ D ( IS = 2.802E-7 N = 0.9521 BV = 44 IBV = 6E-6 RS = 0.1201 CJO = 1.288E-10 VJ = 0.3855 M = 0.4889 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4010EH D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG4010EJ D ( IS = 2.831E-6 N = 0.9816 BV = 44 IBV = 5E-5 RS = 0.1975 CJO = 8.437E-11 VJ = 0.3116 M = 0.4789 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG6010AED D ( IS = 5E-7 N = 0.9751 BV = 66 IBV = 0.0004 RS = 0.3422 CJO = 1.75E-10 VJ = 0.3761 M = 0.4725 FC = 0.5 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PMEG6010CEJ D ( IS = 3.962E-7 N = 0.9774 BV = 66 IBV = 1.1E-5 RS = 0.2033 CJO = 1.103E-01 VJ = 0.3756 M = 0.4916 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
.MODEL PH_PRLL5817 D ( IS = 2.119E-06 N = 1.02 BV = 1000 IBV = 0.001 RS = 0.0419 CJO = 2.52E-10 VJ = 0.4792 M = 0.5104 FC = 500E-3 TT = 0 EG = 0.69 XTI = 2 mfg=Philips type=schottky )
***** PHILIPS *****
***** IRF *****
*LIB\10bq015.spi
.MODEL 10BQ015 d
+IS=1.66692e-05 RS=0.0549971 N=1.0339 EG=0.6
+XTI=0.5 BV=15 IBV=0.001 CJO=4.70891e-10
+VJ=1.5 M=0.699718 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\10bq040.spi
.MODEL 10BQ040 d
+IS=2.13126e-05 RS=0.123203 N=1.53952 EG=0.600841
+XTI=3.78803 BV=40 IBV=0.0001 CJO=1.53747e-10
+VJ=1.5 M=0.476132 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\10bq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on May 13, 98
* MODEL FORMAT: SPICE3
.MODEL 10BQ100 d
+IS=3.8291e-09 RS=100 N=2 EG=0.600259
+XTI=0.5 BV=100 IBV=0.0001 CJO=9.19104e-11
+VJ=1.5 M=0.527626 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\10ctq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Feb  4, 02
* MODEL FORMAT: SPICE3
.MODEL 10CTQ150 d
+IS=1.63362e-06 RS=0.0221615 N=2 EG=0.6
+XTI=0.5 BV=150 IBV=5e-05 CJO=4.60092e-10
+VJ=0.759589 M=0.500823 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\10mq060n.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr  22, 99
* MODEL FORMAT: SPICE3
.MODEL 10MQ060N d
+IS=1e-07 RS=0.142057 N=1.06198 EG=0.6
+XTI=0.5 BV=60 IBV=0.0001 CJO=8.36264e-11
+VJ=1.5 M=0.497422 FC=0.5 TT=1e-09
+KF=0 AF=1


*LIB\10mq100n.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 14, 05
* MODEL FORMAT: SPICE3
.MODEL 10MQ100N d
+IS=1e-07 RS=0.0807081 N=1.65612 EG=0.6
+XTI=0.5 BV=100 IBV=0.00025 CJO=8.62759e-11
+VJ=0.4 M=0.43322 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\10tq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 96
* MODEL FORMAT: SPICE3
.MODEL 10TQ045 d
+IS=9.81804e-08 RS=0.00739225 N=0.993075 EG=0.6
+XTI=0.5 BV=45 IBV=0.0001 CJO=1.42434e-09
+VJ=1.5 M=0.479175 FC=0.5 TT=0
+KF=0 AF=1


*LIB\120lq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar  9, 06
* MODEL FORMAT: SPICE3
.MODEL 120LQ045 d
+IS=5.90313e-09 RS=0.00455345 N=0.737625 EG=1.3
+XTI=0.5 BV=45 IBV=0.0001 CJO=1.29866e-08
+VJ=0.462963 M=0.473356 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\120lq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar  9, 06
* MODEL FORMAT: SPICE3
.MODEL 120LQ100 d
+IS=0.000544678 RS=0.00277937 N=1.83305 EG=0.6
+XTI=0.5 BV=100 IBV=0.0001 CJO=6.48813e-09
+VJ=0.4 M=0.384061 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\12cgq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 12, 00
* MODEL FORMAT: SPICE3
.MODEL 12CGQ150 d
+IS=2.4863e-05 RS=0.0252929 N=2 EG=1.3
+XTI=0.5 BV=150 IBV=0.0001 CJO=6.35956e-10
+VJ=1.5 M=0.562241 FC=0.5 TT=0
+KF=0 AF=1

*LIB\12ctq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 96
* MODEL FORMAT: SPICE3
.MODEL 12CTQ045 d
+IS=5.30534e-09 RS=0.014271 N=0.891364 EG=0.6
+XTI=0.5 BV=45 IBV=0.0001 CJO=7.11199e-10
+VJ=1.5 M=0.484798 FC=0.5 TT=0
+KF=0 AF=1


*LIB\12cwq04fn.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  9, 05
* MODEL FORMAT: SPICE3
.MODEL 12CWQ04FN d
+IS=1.05439e-06 RS=0.0173547 N=1.07052 EG=0.6
+XTI=0.5 BV=40 IBV=0.0001 CJO=1.51803e-09
+VJ=0.4 M=0.516518 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\12tq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 96
* MODEL FORMAT: SPICE3
.MODEL 12TQ045 d
+IS=1.61329e-12 RS=0.01 N=0.5 EG=0.600004
+XTI=0.5 BV=45 IBV=0.0001 CJO=1.59319e-09
+VJ=1.5 M=0.52241 FC=0.5 TT=0
+KF=0 AF=1


*LIB\15cgq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 19, 01
* MODEL FORMAT: SPICE3
.MODEL 15CGQ100 d
+IS=8.74079e-05 RS=0.0180811 N=2 EG=1.3
+XTI=3.01057 BV=100 IBV=0.0001 CJO=1.08792e-09
+VJ=0.846153 M=0.498115 FC=0.5 TT=0
+KF=0 AF=1


*LIB\15clq100.spi
.MODEL 15CLQ100 d
+IS=6.44968e-05 RS=0.014091 N=2 EG=0.996757
+XTI=0.5 BV=100 IBV=0.005 CJO=1.38463e-09
+VJ=0.4 M=0.466344 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\15eth06.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep  27, 05
* MODEL FORMAT: SPICE3
.MODEL 15ETH06 d
+IS=2.2756e-08 RS=0.0177161 N=2 EG=0.6
+XTI=0.500021 BV=600 IBV=0.0001 CJO=1.6387e-10
+VJ=0.71953 M=0.37991 FC=0.5 TT=1e-09
+KF=0 AF=1


*LIB\15ljq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr 12, 01
* MODEL FORMAT: SPICE3
.MODEL 15LJQ100 d
+IS=6.15446e-05 RS=0.0153982 N=1.88088 EG=1.3
+XTI=3.60437 BV=100 IBV=0.0001 CJO=1.08848e-09
+VJ=0.4 M=0.371667 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\160cmq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 01
* MODEL FORMAT: SPICE3
.MODEL 160CMQ045 d
+IS=1.34755e-11 RS=0.00275782 N=0.5 EG=0.6
+XTI=0.5 BV=1000 IBV=0.0001 CJO=4.75072e-09
+VJ=1.5 M=0.542103 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\16cyq150c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 27, 06
* MODEL FORMAT: SPICE3
.MODEL 16CYQ150C d
+IS=1.71508e-05 RS=0.0265393 N=2 EG=1.3
+XTI=2.78486 BV=150 IBV=0.0001 CJO=9.98822e-10
+VJ=0.4 M=0.484035 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\16syq060c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 27, 06
* MODEL FORMAT: SPICE3
.MODEL 16SYQ060C d
+IS=1.66638e-08 RS=0.0183025 N=0.65508 EG=0.6
+XTI=0.5 BV=60 IBV=0.0001 CJO=6.83071e-09
+VJ=0.4 M=0.497741 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\16yq045c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 14, 06
* MODEL FORMAT: SPICE3
.MODEL 16YQ045C d
+IS=4.98611e-07 RS=0.0130029 N=0.98534 EG=1.3
+XTI=2.9591 BV=45 IBV=0.0001 CJO=6.92544e-09
+VJ=0.537519 M=0.490188 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\16yq150c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 14, 06
* MODEL FORMAT: SPICE3
.MODEL 16YQ150C d
+IS=2.63267e-05 RS=0.0169253 N=2 EG=1.3
+XTI=2.95537 BV=150 IBV=0.0001 CJO=1.74923e-09
+VJ=0.4 M=0.470085 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\18tq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 96
* MODEL FORMAT: SPICE3
.MODEL 18TQ045 d
+IS=1.97424e-13 RS=0.00628392 N=0.530234 EG=0.6
+XTI=0.05 BV=45 IBV=0.0001 CJO=8.24939e-09
+VJ=1.5 M=0.462568 FC=0.5 TT=0
+KF=0 AF=1


*LIB\20cjq030.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 27, 96
* MODEL FORMAT: SPICE3
.MODEL 20CJQ030 d
+IS=7.45927e-09 RS=0.0632601 N=0.89875 EG=1.3
+XTI=4 BV=30 IBV=0.0001 CJO=2.9346e-10
+VJ=0.4 M=0.427299 FC=0.5 TT=0
+KF=0 AF=1

*LIB\20clq045.spi
.MODEL 20CLQ045 d
+IS=5.55194e-10 RS=0.01 N=0.736126 EG=0.6
+XTI=0.5 BV=45 IBV=0.005 CJO=2.42073e-09
+VJ=0.470122 M=0.477502 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\20ets12.spi
.MODEL 20ETS12 d
+IS=8.28224e-09 RS=0.00791517 N=1.61051 EG=1.12793
+XTI=0.5 BV=1000 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1
* Model generated on Jan 30, 96
* Model format: SPICE3

*LIB\20ets12a.spi
.MODEL 20ETS12AVG d
+IS=3.14987e-10 RS=0.01 N=1.37516 EG=1.06967
+XTI=4 BV=1200 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1
* Model generated on Apr 26, 96
* Model format: SPICE3

*LIB\20ets12s.spi
.MODEL 20ETS12A+3S d
+IS=2.797e-10 RS=0.0113232 N=1.38813 EG=1.07556
+XTI=4 BV=1200 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1
* Model generated on Apr 26, 96
* Model format: SPICE3

*LIB\22gq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 16, 01
* MODEL FORMAT: SPICE3
.MODEL 22GQ100 d
+IS=5.91885e-14 RS=0.0197462 N=0.527335 EG=0.6
+XTI=0.5 BV=100 IBV=0.0001 CJO=4.67713e-09
+VJ=0.4 M=0.513011 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30cljq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  3, 01
* MODEL FORMAT: SPICE3
.MODEL 30CLJQ045 d
+IS=6.17168e-07 RS=0.0202821 N=1.08809 EG=1.3
+XTI=3.29182 BV=45 IBV=0.0001 CJO=1.24067e-09
+VJ=0.408846 M=0.481835 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30cljq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 16, 01
* MODEL FORMAT: SPICE3
.MODEL 30CLJQ150 d
+IS=1.30646e-06 RS=0.0239928 N=2 EG=1.3
+XTI=3.05712 BV=150 IBV=0.0001 CJO=3.73861e-10
+VJ=0.4 M=0.457852 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30cth02.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 28, 05
* MODEL FORMAT: SPICE3
.MODEL 30CTH02 d
+IS=1e-15 RS=0.01 N=0.77819 EG=1.3
+XTI=4 BV=200 IBV=0.0001 CJO=4.06302e-10
+VJ=0.4 M=0.3385 FC=0.5 TT=1e-07
+KF=0 AF=1

*LIB\30ctq060s.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on May 31, 00
* MODEL FORMAT: SPICE3
.MODEL 30CTQ060S d
+IS=0.001 RS=0.00753336 N=2.31312 EG=0.510131
+XTI=0.497683 BV=60 IBV=0.0001 CJO=1.18606e-09
+VJ=1.5 M=0.494139 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\30eph06.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr 13, 05
* MODEL FORMAT: SPICE3
.MODEL 30EPH06 d
+IS=3.75476e-10 RS=0.0182211 N=2 EG=0.626585
+XTI=0.500695 BV=600 IBV=0.0001 CJO=3.68339e-10
+VJ=1.27928 M=0.404368 FC=0.5 TT=1.23518e-08
+KF=0 AF=1

*LIB\30ljq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  3, 01
* MODEL FORMAT: SPICE3
.MODEL 30LJQ045 d
+IS=3.01029e-08 RS=0.00758833 N=0.877045 EG=0.6
+XTI=0.5 BV=45 IBV=0.0001 CJO=2.65012e-09
+VJ=1.18451 M=0.511241 FC=0.5 TT=0
+KF=0 AF=1


*LIB\30ljq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 21, 01
* MODEL FORMAT: SPICE3
.MODEL 30LJQ100 d
+IS=2.8036e-05 RS=0.0100392 N=2 EG=0.6
+XTI=0.5 BV=100 IBV=0.0001 CJO=1.41531e-09
+VJ=0.4 M=0.47998 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30ljq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  3, 01
* MODEL FORMAT: SPICE3
.MODEL 30LJQ150 d
+IS=4.79361e-06 RS=0.0108545 N=2 EG=1.3
+XTI=0.502388 BV=150 IBV=0.0001 CJO=9.09704e-10
+VJ=0.4 M=0.462283 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30scljq030.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  3, 01
* MODEL FORMAT: SPICE3
.MODEL 30SCLJQ030 d
+IS=3.04923e-06 RS=0.0123656 N=1.0506 EG=1.3
+XTI=2.9944 BV=30 IBV=0.0001 CJO=1.61571e-09
+VJ=0.442068 M=0.472758 FC=0.5 TT=0
+KF=0 AF=1

*LIB\30sljq030.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 16, 01
* MODEL FORMAT: SPICE3
.MODEL 30SLJQ030 d
+IS=2.08649e-07 RS=0.00676047 N=0.86202 EG=0.6
+XTI=0.5 BV=30 IBV=0.0001 CJO=5.85622e-09
+VJ=0.4 M=0.485403 FC=0.5 TT=0
+KF=0 AF=1

*LIB\32ctq030.spi
.MODEL 32CTQ030 d
+IS=2.21746e-11 RS=0.01 N=0.5 EG=0.6
+XTI=2.38672 BV=30 IBV=0.00175 CJO=2.11811e-09
+VJ=1.5 M=0.499425 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\32ctq030h.spi
.MODEL 32CTQ030H d
+IS=1e-15 RS=0.01 N=0.5 EG=1.07785
+XTI=4 BV=30 IBV=0.00175 CJO=2.11811e-09
+VJ=1.5 M=0.499425 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\35cgq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar  8, 01
* MODEL FORMAT: SPICE3
.MODEL 35CGQ100 d
+IS=1e-15 RS=0.01681 N=0.5 EG=0.608064
+XTI=0.500208 BV=100 IBV=0.0001 CJO=2.00581e-09
+VJ=1.24629 M=0.513186 FC=0.5 TT=1e-09
+KF=0 AF=1



*LIB\35clq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 19, 01
* MODEL FORMAT: SPICE3
.MODEL 35CLQ045 d
+IS=2.76847e-07 RS=0.00674255 N=1.0155 EG=1.3
+XTI=4 BV=45 IBV=0.0001 CJO=2.76301e-09
+VJ=1.01389 M=0.489865 FC=0.5 TT=0
+KF=0 AF=1

*LIB\40cpq060.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Jan 17, 02
* MODEL FORMAT: SPICE3
.MODEL 40CPQ050 d
+IS=2.4532e-11 RS=0.0071 N=0.5 EG=0.6
+XTI=0.5 BV=1000 IBV=0.0001 CJO=2.49633e-09
+VJ=1.5 M=0.483473 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\40ctq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 14, 05
* MODEL FORMAT: SPICE3
.MODEL 40CTQ045 d
+IS=3.357e-08 RS=0.01 N=0.5 EG=1.04653
+XTI=0.957426 BV=45 IBV=0.00025 CJO=1.51919e-08
+VJ=0.4 M=0.704417 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\40eps08.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 28, 96
* MODEL FORMAT: SPICE3
.MODEL 40EPS08 d
+IS=1e-15 RS=0.00426912 N=0.926332 EG=0.6
+XTI=0.5 BV=800 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\40eps12.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 28, 96
* MODEL FORMAT: SPICE3
.MODEL 40EPS12 d
+IS=1e-15 RS=0.00426912 N=0.926332 EG=0.6
+XTI=0.5 BV=1200 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\40eps16.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 28, 96
* MODEL FORMAT: SPICE3
.MODEL 40EPS16 d
+IS=1e-15 RS=0.00426912 N=0.926332 EG=0.6
+XTI=0.5 BV=1600 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\50wq06fn.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr  1, 99
* MODEL FORMAT: SPICE3
.MODEL 50WQ06FN d
+IS=1e-15 RS=0.0205874 N=0.5 EG=1.3
+XTI=0.5 BV=1000 IBV=0.0001 CJO=8.86241e-10
+VJ=0.899259 M=0.559144 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\5eq100.spi
.MODEL 5EQ100 d
+IS=8.77154e-05 RS=0.0202145 N=2 EG=0.815312
+XTI=3.9995 BV=100 IBV=0.005 CJO=1.06148e-09
+VJ=0.79108 M=0.475554 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\60lq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 19, 01
* MODEL FORMAT: SPICE3
.MODEL 60LQ045 d
+IS=1e-07 RS=0.00252226 N=0.914851 EG=0.6
+XTI=0.5 BV=45 IBV=0.0001 CJO=6.87655e-09
+VJ=0.4 M=0.408789 FC=0.5 TT=0
+KF=0 AF=1

*LIB\60lq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 16, 01
* MODEL FORMAT: SPICE3
.MODEL 60LQ100 d
+IS=0.001 RS=0.0026041 N=1.79037 EG=0.6
+XTI=0.5 BV=100 IBV=0.0001 CJO=4.12278e-09
+VJ=0.4 M=0.477205 FC=0.5 TT=0
+KF=0 AF=1

*LIB\6cwq04fn.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 12, 05
* MODEL FORMAT: SPICE3
.MODEL 6CWQ04FN d
+IS=7.48131e-13 RS=0.0287717 N=0.540086 EG=0.6
+XTI=0.5 BV=40 IBV=0.0001 CJO=5.09354e-10
+VJ=0.795245 M=0.513157 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\6cwq10fn.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Feb 15, 02
* MODEL FORMAT: SPICE3
.MODEL 6CWQ10FN d
+IS=1.92816e-06 RS=0.0227346 N=2 EG=0.6
+XTI=0.5 BV=100 IBV=0.001 CJO=2.9028e-10
+VJ=0.4 M=0.453836 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\6tq045.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Sep 17, 96
* MODEL FORMAT: SPICE3
.MODEL 6TQ045 d
+IS=1.1357e-08 RS=0.0148614 N=0.895316 EG=1.3
+XTI=4 BV=45 IBV=0.0001 CJO=7.53573e-10
+VJ=1.5 M=0.502931 FC=0.5 TT=0
+KF=0 AF=1


*LIB\75lq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 20, 01
* MODEL FORMAT: SPICE3
.MODEL 75LQ150 d
+IS=6.47147e-05 RS=0.00457083 N=2 EG=0.6
+XTI=0.5 BV=150 IBV=0.0001 CJO=3.61923e-09
+VJ=0.4 M=0.479638 FC=0.5 TT=0
+KF=0 AF=1

*LIB\75slq030.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec  3, 01
* MODEL FORMAT: SPICE3
.MODEL 75SLQ030 d
+IS=1.05375e-05 RS=0.00235787 N=0.994404 EG=1.3
+XTI=0.5 BV=30 IBV=0.0001 CJO=1.14291e-08
+VJ=0.4 M=0.46991 FC=0.5 TT=0
+KF=0 AF=1

*LIB\80clq150.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 19, 01
* MODEL FORMAT: SPICE3
.MODEL 80CLQ150 d
+IS=3.00965e-05 RS=0.00595685 N=2 EG=1.3
+XTI=3.40773 BV=150 IBV=0.0001 CJO=1.45286e-09
+VJ=0.4 M=0.415374 FC=0.5 TT=0
+KF=0 AF=1

*LIB\80ebu02.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr  2, 02
* MODEL FORMAT: SPICE3
.MODEL 80EBU02 d
+IS=6.10239e-06 RS=0.00151476 N=2 EG=0.1
+XTI=0.0005 BV=200 IBV=5e-05 CJO=1.77691e-09
+VJ=0.4 M=0.495417 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\8eq045.spi
.MODEL 8EQ045 d
+IS=1.8026e-05 RS=0.0138308 N=1.50131 EG=0.689509
+XTI=4 BV=45 IBV=0.005 CJO=1.98488e-09
+VJ=0.711167 M=0.477336 FC=0.5 TT=0
+KF=0 AF=1
* Model generated on May 28, 96
* Model format: SPICE3

*LIB\8eth06.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct  17, 05
* MODEL FORMAT: SPICE3
.MODEL 8ETH06 d
+IS=6.92843e-10 RS=0.121017 N=2 EG=1.3
+XTI=0.528448 BV=600 IBV=0.0001 CJO=1.56732e-10
+VJ=0.4 M=0.404011 FC=0.5 TT=1e-09
+KF=0 AF=1


*LIB\8ews08.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 25, 96
* MODEL FORMAT: SPICE3
.MODEL 8EWS08 d
+IS=1.04304e-07 RS=0.0103888 N=2 EG=1.28885
+XTI=3.00461 BV=800 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\8ews10.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 25, 96
* MODEL FORMAT: SPICE3
.MODEL 8EWS10 d
+IS=1.17378e-07 RS=0.0104837 N=2 EG=1.29966
+XTI=3.06473 BV=1000 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\8ews12.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 25, 96
* MODEL FORMAT: SPICE3
.MODEL 8EWS12 d
+IS=1e-07 RS=0.0115955 N=1.9747 EG=0.6
+XTI=0.5 BV=1200 IBV=0.0001 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\90clq100.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 20, 01
* MODEL FORMAT: SPICE3
.MODEL 90CLQ100 d
+IS=0.00032603 RS=0.00931445 N=2 EG=1.3
+XTI=0.5 BV=100 IBV=0.0001 CJO=3.07785e-09
+VJ=0.4 M=0.479989 FC=0.5 TT=0
+KF=0 AF=1

*LIB\d200td120u.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Oct 17, 01
* MODEL FORMAT: SPICE3
.MODEL 200TD120U d
+IS=1.4976e-11 RS=0.007312 N=2 EG=0.6
+XTI=4 BV=1200 IBV=0.0001 CJO=1.8e-09
+VJ=0.4 M=0.45418 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfa06tb120.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on May  8, 01
* MODEL FORMAT: SPICE3
.MODEL HFA06TB120 d
+IS=0.001 RS=0.110401 N=13.6537 EG=0.6
+XTI=0.5 BV=1200 IBV=0.0001 CJO=1.1896e-10
+VJ=0.4 M=0.430052 FC=0.5 TT=5.54521e-08
+KF=0 AF=1

*LIB\hfa08tb60.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Jan 30, 02
* MODEL FORMAT: SPICE3
.MODEL HFA08TB60 d
+IS=2.88464e-12 RS=0.0305193 N=2 EG=1.29955
+XTI=0.521907 BV=600 IBV=0.0001 CJO=1.37419e-10
+VJ=0.4 M=0.418241 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfa140nh60r.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Jan 17, 02
* MODEL FORMAT: SPICE3
.MODEL HFA140NH60R d
+IS=2.34895e-06 RS=0.0025 N=2 EG=1.3
+XTI=0.5 BV=1000 IBV=0.0001 CJO=4.67077e-09
+VJ=0.4 M=0.467713 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfa15pb60.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 10, 01
* MODEL FORMAT: SPICE3
.MODEL HFA15PB60 d
+IS=7.68701e-11 RS=0.020004 N=2 EG=0.6
+XTI=0.5 BV=600 IBV=0.0001 CJO=2.94798e-10
+VJ=0.7742 M=0.447397 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfa30pa60c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on May 31, 00
* MODEL FORMAT: SPICE3
.MODEL HFA30PA60C d
+IS=0.000690394 RS=0.0117897 N=6.00599 EG=0.6
+XTI=0.5 BV=600 IBV=0.0001 CJO=4.84089e-11
+VJ=4720.92 M=0.9 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfa30ta60cs.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Apr  7, 05
* MODEL FORMAT: SPICE3
.MODEL HFA30TA60CS d
+IS=0.001 RS=0.0395 N=2 EG=1.282
+XTI=3.02161 BV=600 IBV=0.0001 CJO=2.73039e-10
+VJ=1.5 M=0.451856 FC=0.5 TT=2.42596e-08
+KF=0 AF=1

*LIB\hfa80nc40csl.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar 10, 00
* MODEL FORMAT: SPICE3
.MODEL HFA80NC40CSL d
+IS=2.37825e-07 RS=0.01 N=2 EG=1.04775
+XTI=2.97132 BV=400 IBV=0.0001 CJO=1.50848e-09
+VJ=0.4 M=0.453789 FC=0.5 TT=1e-09
+KF=0 AF=1


*LIB\hfb16hy20c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 10, 01
* MODEL FORMAT: SPICE3
.MODEL HFB16HY20C d
+IS=3.69563e-06 RS=0.0218406 N=2 EG=0.6
+XTI=0.500087 BV=200 IBV=0.0001 CJO=1.17122e-09
+VJ=0.4 M=0.337217 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb20hj20c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 29, 01
* MODEL FORMAT: SPICE3
.MODEL HFB20HJ20C d
+IS=2.31797e-07 RS=0.0180424 N=2 EG=1.3
+XTI=3.00177 BV=200 IBV=0.0001 CJO=1.25047e-10
+VJ=0.4 M=0.329663 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb25hj20.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 30, 01
* MODEL FORMAT: SPICE3
.MODEL HFB25HJ20 d
+IS=5.77437e-07 RS=0.00510648 N=2 EG=1.3
+XTI=2.94572 BV=200 IBV=0.0001 CJO=4.64754e-10
+VJ=0.4 M=0.332685 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb35hb20c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 10, 01
* MODEL FORMAT: SPICE3
.MODEL HFB35HB20C d
+IS=3.09007e-07 RS=0.012861 N=2 EG=1.3
+XTI=3.0157 BV=200 IBV=0.0001 CJO=1.14597e-09
+VJ=0.4 M=0.389409 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb50hc20.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Dec 10, 01
* MODEL FORMAT: SPICE3
.MODEL HFB50HC20 d
+IS=7.18041e-06 RS=0.00862324 N=2 EG=1.3
+XTI=2.22389 BV=200 IBV=0.0001 CJO=2.80175e-09
+VJ=0.4 M=0.361761 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb60hf20.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Nov 30, 01
* MODEL FORMAT: SPICE3
.MODEL HFB60HF20 d
+IS=1.33655e-05 RS=0.00424093 N=2 EG=0.6
+XTI=0.5 BV=200 IBV=0.0001 CJO=1.42712e-09
+VJ=0.4 M=0.358042 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\hfb60hf20c.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on Mar  6, 03
* MODEL FORMAT: SPICE3
.MODEL HFB60HF20C d
+IS=8.824e-07 RS=0.0053362 N=2 EG=1.3
+XTI=2.93114 BV=200 IBV=0.0001 CJO=9.80264e-10
+VJ=0.4 M=0.349795 FC=0.5 TT=1e-09
+KF=0 AF=1

*LIB\irkd235.spi
.MODEL IRKD235 d
+IS=7.75629e-16 RS=0.46044 N=1.09796 EG=1.23653
+XTI=3.30648 BV=2200 IBV=0.05 CJO=1e-11
+VJ=0.7 M=0.5 FC=0.5 TT=1e-09
+KF=0 AF=1
* Model generated on Jun  3, 96
* Model format: SPICE3

*LIB\mbr6045wt.spi
**************************************
*      Model Generated by MODPEX     *
*Copyright(c) Symmetry Design Systems*
*         All Rights Reserved        *
*    UNPUBLISHED LICENSED SOFTWARE   *
*   Contains Proprietary Information *
*      Which is The Property of      *
*     SYMMETRY OR ITS LICENSORS      *
*Commercial Use or Resale Restricted *
*   by Symmetry License Agreement    *
**************************************
* Model generated on May 31, 00
* MODEL FORMAT: SPICE3
.MODEL MBR6045WT d
+IS=0.000193712 RS=0.0036073 N=1.64274 EG=1.3
+XTI=0.5 BV=45 IBV=0.0001 CJO=4.10772e-09
+VJ=0.640163 M=0.517178 FC=0.5 TT=1e-09
+KF=0 AF=1

***** IRF *****
